### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.1 (WebPack) - M.53d | Target Family: | Spartan3E
OS Platform: | NT | Target Device: | xc3s250e
Project ID (random number) | 684acf2150724198a130877b888bb684.7e7c5fed29984f83a57e6c11327bf53b.2 | Target Package: | pq208
Registration ID | 176036481_0_0_631 | Target Speed: | -4
Date Generated | 2012-05-05T23:19:20 | Tool Flow | CommandLine

User Environment
OS Name | Microsoft Windows XP Professional | OS Release | Service Pack 3 (build 2600)
CPU Name | Intel(R) Xeon(R) CPU W3520 @ 2.67GHz | CPU Speed | 2666 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
| MiscellaneousStatistics AGG_BONDED_IO=94 AGG_IO=94 AGG_SLICE=2403 NUM_4_INPUT_LUT=3968 NUM_BONDED_IBUF=27 NUM_BONDED_IOB=67 NUM_BUFGMUX=9 NUM_CYMUX=611 NUM_DCM=1 NUM_DP_RAM=64 NUM_IOB_FF=12 NUM_IOB_LATCH=8 NUM_LUT_RT=123 NUM_RAMB16=2 NUM_SLICEL=2355 NUM_SLICEM=48 NUM_SLICE_FF=1735 NUM_XOR=300 | NetStatistics NumNets_Active=4607 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BRAMADDR=20 NumNodesOfType_Active_BRAMDUMMY=64 NumNodesOfType_Active_CLKPIN=1061 NumNodesOfType_Active_CNTRLPIN=1467 NumNodesOfType_Active_DOUBLE=10173 NumNodesOfType_Active_DUMMY=12218 NumNodesOfType_Active_DUMMYBANK=34 NumNodesOfType_Active_DUMMYESC=12 NumNodesOfType_Active_GLOBAL=315 NumNodesOfType_Active_HFULLHEX=101 NumNodesOfType_Active_HLONG=19 NumNodesOfType_Active_HUNIHEX=537 NumNodesOfType_Active_INPUT=13600 NumNodesOfType_Active_IOBOUTPUT=24 NumNodesOfType_Active_OMUX=4427 NumNodesOfType_Active_OUTPUT=4447 NumNodesOfType_Active_PREBXBY=3468 NumNodesOfType_Active_VFULLHEX=486 NumNodesOfType_Active_VLONG=99 NumNodesOfType_Active_VUNIHEX=563 NumNodesOfType_Vcc_BRAMDUMMY=2 NumNodesOfType_Vcc_CLKPIN=1 NumNodesOfType_Vcc_CNTRLPIN=11 NumNodesOfType_Vcc_DUMMYBANK=3 NumNodesOfType_Vcc_INPUT=36 NumNodesOfType_Vcc_PREBXBY=21 NumNodesOfType_Vcc_VCCOUT=39 SiteStatistics IBUF-DIFFM=3 IBUF-DIFFMI=3 IBUF-DIFFS=11 IBUF-DIFFSI=3 IBUF-IOB=1 IOB-DIFFM=33 IOB-DIFFS=32 SLICEL-SLICEM=1151 | SiteSummary BUFGMUX=9 BUFGMUX_GCLKMUX=9 BUFGMUX_GCLK_BUFFER=9 DCM=1 DCM_DCM=1 IBUF=27 IBUF_IFD_DELAY=2 IBUF_IFF1=2 IBUF_INBUF=27 IBUF_PAD=27 IOB=67 IOB_IFD_DELAY=9 IOB_IFF1=9 IOB_IFF2=1 IOB_INBUF=11 IOB_OFF1=8 IOB_OUTBUF=67 IOB_PAD=67 RAMB16=2 RAMB16_RAMB16=2 RAMB16_RAMB16A=2 SLICEL=2355 SLICEL_C1VDD=36 SLICEL_C2VDD=30 SLICEL_CYMUXF=311 SLICEL_CYMUXG=300 SLICEL_F=1966 SLICEL_F5MUX=186 SLICEL_F6MUX=12 SLICEL_FFX=907 SLICEL_FFY=812 SLICEL_G=1906 SLICEL_GNDF=101 SLICEL_GNDG=100 SLICEL_XORF=149 SLICEL_XORG=151 SLICEM=48 SLICEM_F=48 SLICEM_F5MUX=16 SLICEM_F6MUX=16 SLICEM_FFY=16 SLICEM_G=48 SLICEM_WSGEN=32

Configuration Data
BUFGMUX S=[S_INV:9] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:9] S=[S_INV:9] [S:0] DCM PSCLK=[PSCLK_INV:1] [PSCLK:0] PSEN=[PSEN_INV:1] [PSEN:0] PSINCDEC=[PSINCDEC_INV:1] [PSINCDEC:0] RST=[RST:1] [RST_INV:0] DCM_DCM CLKDV_DIVIDE=[2:1] CLKOUT_PHASE_SHIFT=[NONE:1] CLK_FEEDBACK=[1X:1] DESKEW_ADJUST=[7:1] DFS_FREQUENCY_MODE=[LOW:1] DLL_FREQUENCY_MODE=[LOW:1] DUTY_CYCLE_CORRECTION=[TRUE:1] FACTORY_JF1=[0XC0:1] FACTORY_JF2=[0X80:1] PSCLK=[PSCLK_INV:1] [PSCLK:0] PSEN=[PSEN_INV:1] [PSEN:0] PSINCDEC=[PSINCDEC_INV:1] [PSINCDEC:0] RST=[RST:1] [RST_INV:0] IBUF ICLK1=[ICLK1_INV:0] [ICLK1:2] IBUF_IFF1 CK=[CK:2] [CK_INV:0] IFF1_INIT_ATTR=[INIT0:2] LATCH_OR_FF=[FF:2] IBUF_INBUF IFD_DELAY_VALUE=[DLY3:2] IBUF_PAD IOATTRBOX=[LVCMOS25:27] PULL=[PULLUP:3] IOB ICLK1=[ICLK1_INV:8] [ICLK1:1] ICLK2=[ICLK2_INV:0] [ICLK2:1] O1=[O1_INV:0] [O1:67] OCE=[OCE:8] [OCE_INV:0] OTCLK1=[OTCLK1_INV:0] [OTCLK1:8] SR=[SR:1] [SR_INV:8] T1=[T1_INV:2] [T1:26] | IOB_IFF1 CK=[CK:1] [CK_INV:8] IFF1_INIT_ATTR=[INIT0:9] IFF1_SR_ATTR=[SRLOW:1] IFFATTRBOX=[SYNC:1] LATCH_OR_FF=[FF:1] [LATCH:8] SR=[SR:1] [SR_INV:0] IOB_IFF2 CK=[CK:1] [CK_INV:0] IFF2_INIT_ATTR=[INIT0:1] IFF2_SR_ATTR=[SRLOW:1] IFFATTRBOX=[SYNC:1] LATCH_OR_FF=[FF:1] SR=[SR:1] [SR_INV:0] IOB_INBUF IFD_DELAY_VALUE=[DLY3:9] IOB_OFF1 CE=[CE:8] [CE_INV:0] CK=[CK:8] [CK_INV:0] D=[D:8] [D_INV:0] LATCH_OR_FF=[FF:8] OFF1_INIT_ATTR=[INIT0:8] OFF1_SR_ATTR=[SRLOW:8] OFFATTRBOX=[SYNC:8] SR=[SR:0] [SR_INV:8] IOB_OUTBUF IN=[IN_INV:0] [IN:67] TRI=[TRI_INV:2] [TRI:26] IOB_PAD DRIVEATTRBOX=[12:67] IOATTRBOX=[LVCMOS25:67] PULL=[PULLUP:12] SLEW=[SLOW:67] RAMB16 CLKA=[CLKA_INV:0] [CLKA:2] ENA=[ENA_INV:0] [ENA:2] SSRA=[SSRA_INV:0] [SSRA:2] WEA=[WEA:2] [WEA_INV:0] | RAMB16_RAMB16A CLKA=[CLKA_INV:0] [CLKA:2] ENA=[ENA_INV:0] [ENA:2] PORTA_ATTR=[1024X18:2] SSRA=[SSRA_INV:0] [SSRA:2] WEA=[WEA:2] [WEA_INV:0] WRITEMODEA=[WRITE_FIRST:2] SLICEL BX=[BX_INV:0] [BX:560] BY=[BY:380] [BY_INV:12] CE=[CE:699] [CE_INV:38] CIN=[CIN_INV:0] [CIN:275] CLK=[CLK:967] [CLK_INV:38] SR=[SR:498] [SR_INV:155] SLICEL_CYMUXF 0=[0:311] [0_INV:0] 1=[1_INV:0] [1:311] SLICEL_CYMUXG 0=[0:300] [0_INV:0] SLICEL_F5MUX S0=[S0:186] [S0_INV:0] SLICEL_F6MUX S0=[S0:12] [S0_INV:0] SLICEL_FFX CE=[CE:646] [CE_INV:33] CK=[CK:888] [CK_INV:19] D=[D:907] [D_INV:0] FFX_INIT_ATTR=[INIT0:855] [INIT1:52] FFX_SR_ATTR=[SRLOW:861] [SRHIGH:46] LATCH_OR_FF=[FF:907] REV=[REV_INV:0] [REV:67] SR=[SR:461] [SR_INV:132] SYNC_ATTR=[ASYNC:458] [SYNC:449] SLICEL_FFY CE=[CE:616] [CE_INV:36] CK=[CK:774] [CK_INV:38] D=[D:800] [D_INV:12] FFY_INIT_ATTR=[INIT0:792] [INIT1:20] FFY_SR_ATTR=[SRLOW:793] [SRHIGH:19] LATCH_OR_FF=[FF:812] REV=[REV_INV:0] [REV:1] SR=[SR:425] [SR_INV:69] SYNC_ATTR=[ASYNC:412] [SYNC:400] | SLICEL_XORF 1=[1_INV:0] [1:149] SLICEM BX=[BX_INV:0] [BX:16] BY=[BY:48] [BY_INV:0] CLK=[CLK:32] [CLK_INV:0] SR=[SR:32] [SR_INV:0] SLICEM_F DI=[DI:32] [DI_INV:0] F_ATTR=[DUAL_PORT:32] LUT_OR_MEM=[LUT:16] [RAM:32] SLICEM_F5MUX S0=[S0:16] [S0_INV:0] SLICEM_F6MUX S0=[S0:16] [S0_INV:0] SLICEM_FFY CK=[CK:16] [CK_INV:0] D=[D:16] [D_INV:0] FFY_INIT_ATTR=[INIT0:16] FFY_SR_ATTR=[SRLOW:16] LATCH_OR_FF=[FF:16] SYNC_ATTR=[ASYNC:16] SLICEM_G DI=[DI:32] [DI_INV:0] G_ATTR=[DUAL_PORT:32] LUT_OR_MEM=[LUT:16] [RAM:32] SLICEM_WSGEN CK=[CK:32] [CK_INV:0] SYNC_ATTR=[ASYNC:16] WE=[WE_INV:0] [WE:32]

Pin Data
BUFGMUX I0=9 O=9 S=9 BUFGMUX_GCLKMUX I0=9 OUT=9 S=9 BUFGMUX_GCLK_BUFFER IN=9 OUT=9 DCM CLK0=1 CLKFB=1 CLKFX=1 CLKIN=1 LOCKED=1 PSCLK=1 PSEN=1 PSINCDEC=1 RST=1 DCM_DCM CLK0=1 CLKFB=1 CLKFX=1 CLKIN=1 LOCKED=1 PSCLK=1 PSEN=1 PSINCDEC=1 RST=1 IBUF I=25 ICLK1=2 IQ1=2 PAD=27 IBUF_IFD_DELAY IN=2 OUT=2 IBUF_IFF1 CK=2 D=2 Q=2 IBUF_INBUF IN=27 OUT=27 IBUF_PAD PAD=27 IOB I=3 ICLK1=9 ICLK2=1 IQ1=9 IQ2=1 O1=67 OCE=8 OTCLK1=8 PAD=67 SR=9 T1=28 IOB_IFD_DELAY IN=9 OUT=9 IOB_IFF1 CK=9 D=9 Q=9 SR=1 IOB_IFF2 CK=1 D=1 Q=1 SR=1 IOB_INBUF IN=11 OUT=11 IOB_OFF1 CE=8 CK=8 D=8 Q=8 SR=8 IOB_OUTBUF IN=67 OUT=67 TRI=28 IOB_PAD PAD=67 RAMB16 ADDRA10=2 ADDRA11=2 ADDRA12=2 ADDRA13=2 ADDRA4=2 ADDRA5=2 ADDRA6=2 ADDRA7=2 ADDRA8=2 ADDRA9=2 CLKA=2 DIA0=2 DIA1=2 DIA10=2 DIA11=2 DIA12=2 DIA13=2 DIA14=2 DIA15=2 DIA2=2 DIA3=2 DIA4=2 DIA5=2 DIA6=2 DIA7=2 DIA8=2 DIA9=2 DIPA0=2 DIPA1=2 DOA0=2 DOA1=2 DOA10=2 DOA11=2 DOA12=2 DOA13=2 DOA14=1 DOA15=1 DOA2=2 DOA3=2 DOA4=2 DOA5=2 DOA6=2 DOA7=2 DOA8=2 DOA9=2 DOPA0=1 DOPA1=1 ENA=2 SSRA=2 WEA=2 | RAMB16_RAMB16 ADDRA=2 DIA=2 DOA=2 RAMB16_RAMB16A ADDRA=2 ADDRA10=2 ADDRA11=2 ADDRA12=2 ADDRA13=2 ADDRA4=2 ADDRA5=2 ADDRA6=2 ADDRA7=2 ADDRA8=2 ADDRA9=2 CLKA=2 DIA=2 DIA0=2 DIA1=2 DIA10=2 DIA11=2 DIA12=2 DIA13=2 DIA14=2 DIA15=2 DIA2=2 DIA3=2 DIA4=2 DIA5=2 DIA6=2 DIA7=2 DIA8=2 DIA9=2 DIPA0=2 DIPA1=2 DOA=2 DOA0=2 DOA1=2 DOA10=2 DOA11=2 DOA12=2 DOA13=2 DOA14=1 DOA15=1 DOA2=2 DOA3=2 DOA4=2 DOA5=2 DOA6=2 DOA7=2 DOA8=2 DOA9=2 DOPA0=1 DOPA1=1 ENA=2 SSRA=2 WEA=2 SLICEL BX=560 BY=392 CE=737 CIN=275 CLK=1005 COUT=300 F1=1963 F2=1881 F3=1391 F4=878 F5=24 FX=8 FXINA=12 FXINB=12 G1=1905 G2=1819 G3=1297 G4=746 SR=653 X=1204 XQ=907 Y=1078 YQ=812 | SLICEL_C1VDD 1=36 SLICEL_C2VDD 1=30 SLICEL_CYMUXF 0=311 1=311 OUT=311 S0=311 SLICEL_CYMUXG 0=300 1=300 OUT=300 S0=300 SLICEL_F A1=1963 A2=1881 A3=1391 A4=878 D=1966 SLICEL_F5MUX F=186 G=186 OUT=186 S0=186 SLICEL_F6MUX 0=12 1=12 OUT=12 S0=12 SLICEL_FFX CE=679 CK=907 D=907 Q=907 REV=67 SR=593 SLICEL_FFY CE=652 CK=812 D=812 Q=812 REV=1 SR=494 SLICEL_G A1=1905 A2=1819 A3=1297 A4=746 D=1906 SLICEL_GNDF 0=101 SLICEL_GNDG 0=100 SLICEL_XORF 0=149 1=149 O=149 SLICEL_XORG 0=151 1=151 O=151 SLICEM BX=16 BY=48 CLK=32 F1=48 F2=48 F3=48 F4=37 F5=16 FX=8 FXINA=16 FXINB=16 G1=48 G2=48 G3=48 G4=43 SR=32 X=32 Y=24 YQ=16 SLICEM_F A1=48 A2=48 A3=48 A4=37 D=48 DI=32 WF1=32 WF2=32 WF3=32 WF4=32 WS=32 | SLICEM_F5MUX F=16 G=16 OUT=16 S0=16 SLICEM_F6MUX 0=16 1=16 OUT=16 S0=16 SLICEM_FFY CK=16 D=16 Q=16 SLICEM_G A1=48 A2=48 A3=48 A4=43 D=32 DI=32 WG1=32 WG2=32 WG3=32 WG4=32 WS=32 SLICEM_WSGEN CK=32 WE=32 WSF=32 WSG=32

Software Quality
Run Statistics
Bitgen | 814 | 815 | 0 | 0 | 0 | 0 | 0
MAP | 419 | 419 | 0 | 0 | 0 | 0 | 0
NGDBuild | 434 | 433 | 0 | 0 | 0 | 0 | 0
PAR | 419 | 410 | 8 | 0 | 0 | 0 | 0
_impact | 172 | 163 | 0 | 0 | 0 | 0 | 0
arwz | 47 | 47 | 0 | 0 | 0 | 0 | 0
bitgen | 128 | 128 | 0 | 0 | 0 | 0 | 0
compxlib | 11 | 11 | 0 | 0 | 0 | 0 | 0
edif2ngd | 6189 | 6189 | 0 | 0 | 0 | 0 | 0
map | 133 | 130 | 0 | 0 | 0 | 0 | 0
ngc2edif | 5 | 5 | 0 | 0 | 0 | 0 | 0
ngdbuild | 159 | 159 | 0 | 0 | 0 | 0 | 0
par | 130 | 127 | 3 | 0 | 0 | 0 | 0
trce | 536 | 536 | 0 | 0 | 0 | 0 | 0
xawinfo | 15 | 15 | 0 | 0 | 0 | 0 | 0
xps | 1 | 1 | 0 | 0 | 0 | 0 | 0
xst | 560 | 557 | 0 | 0 | 0 | 0 | 0

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUF=8 | NGDBUILD_NUM_BUFG=6 | NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FD=11
NGDBUILD_NUM_FDC=3 | NGDBUILD_NUM_FDCE=8 | NGDBUILD_NUM_FDE=302 | NGDBUILD_NUM_FDP=1
NGDBUILD_NUM_FDPE=2 | NGDBUILD_NUM_FDR=4 | NGDBUILD_NUM_FDRE=142 | NGDBUILD_NUM_FDRS=2
NGDBUILD_NUM_FDR_1=8 | NGDBUILD_NUM_FDS=1 | NGDBUILD_NUM_FDSE=53 | NGDBUILD_NUM_FDS_1=2
NGDBUILD_NUM_GND=7 | NGDBUILD_NUM_IBUF=8 | NGDBUILD_NUM_IBUFG=4 | NGDBUILD_NUM_INV=29
NGDBUILD_NUM_IOBUF=11 | NGDBUILD_NUM_LD=8 | NGDBUILD_NUM_LUT1=16 | NGDBUILD_NUM_LUT2=397
NGDBUILD_NUM_LUT2_D=32 | NGDBUILD_NUM_LUT2_L=17 | NGDBUILD_NUM_LUT3=504 | NGDBUILD_NUM_LUT3_D=39
NGDBUILD_NUM_LUT3_L=37 | NGDBUILD_NUM_LUT4=1058 | NGDBUILD_NUM_LUT4_D=79 | NGDBUILD_NUM_LUT4_L=150
NGDBUILD_NUM_MUXCY=67 | NGDBUILD_NUM_MUXF5=194 | NGDBUILD_NUM_MUXF6=20 | NGDBUILD_NUM_MUXF7=8
NGDBUILD_NUM_OBUF=39 | NGDBUILD_NUM_OBUFT=17 | NGDBUILD_NUM_RAM16X1D=32 | NGDBUILD_NUM_VCC=5
NGDBUILD_NUM_XORCY=72
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUF=8 | NGDBUILD_NUM_BUFG=9 | NGDBUILD_NUM_DCM_SP=1 | NGDBUILD_NUM_FD=79
NGDBUILD_NUM_FDC=14 | NGDBUILD_NUM_FDCE=155 | NGDBUILD_NUM_FDCE_1=8 | NGDBUILD_NUM_FDCP=64
NGDBUILD_NUM_FDC_1=6 | NGDBUILD_NUM_FDE=547 | NGDBUILD_NUM_FDP=12 | NGDBUILD_NUM_FDPE=5
NGDBUILD_NUM_FDR=172 | NGDBUILD_NUM_FDRE=612 | NGDBUILD_NUM_FDRE_1=32 | NGDBUILD_NUM_FDRS=2
NGDBUILD_NUM_FDRSE=2 | NGDBUILD_NUM_FDR_1=8 | NGDBUILD_NUM_FDS=1 | NGDBUILD_NUM_FDSE=53
NGDBUILD_NUM_FDS_1=2 | NGDBUILD_NUM_GND=12 | NGDBUILD_NUM_IBUF=33 | NGDBUILD_NUM_IBUFG=5
NGDBUILD_NUM_INV=38 | NGDBUILD_NUM_LD=8 | NGDBUILD_NUM_LUT1=137 | NGDBUILD_NUM_LUT1_L=11
NGDBUILD_NUM_LUT2=878 | NGDBUILD_NUM_LUT2_D=32 | NGDBUILD_NUM_LUT2_L=152 | NGDBUILD_NUM_LUT3=704
NGDBUILD_NUM_LUT3_D=39 | NGDBUILD_NUM_LUT3_L=357 | NGDBUILD_NUM_LUT4=1342 | NGDBUILD_NUM_LUT4_D=79
NGDBUILD_NUM_LUT4_L=292 | NGDBUILD_NUM_MUXCY=91 | NGDBUILD_NUM_MUXCY_L=520 | NGDBUILD_NUM_MUXF5=202
NGDBUILD_NUM_MUXF6=20 | NGDBUILD_NUM_MUXF7=8 | NGDBUILD_NUM_OBUF=39 | NGDBUILD_NUM_OBUFT=28
NGDBUILD_NUM_PULLUP=15 | NGDBUILD_NUM_RAMB16_S18=2 | NGDBUILD_NUM_TS_TIMESPEC=1 | NGDBUILD_NUM_VCC=12
NGDBUILD_NUM_XORCY=300