Release 12.1 - par M.53d (nt)
Copyright (c) 1995-2010 Xilinx, Inc.  All rights reserved.

Sat May 05 23:18:49 2012


INFO: The IO information is provided in three file formats as part of the Place and Route (PAR) process.  These formats are:
1. The <design name>_pad.txt file (this file) designed to provide information on IO usage in a human readable ASCII text format viewable through common text editors.
2. The <design namd>_pad.csv file for use with spreadsheet programs such as MS Excel. This file can also be read by PACE to communicate post PAR IO information.
3. The <design name>.pad file designed for parsing by customers.  It uses the "|" as a data field separator.

INPUT FILE:       pba03_fpga_map.ncd
OUTPUT FILE:      pba03_fpga_pad.txt
PART TYPE:        xc3s250e
SPEED GRADE:      -4
PACKAGE:          pq208

Pinout by Pin Number:

+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|Pin Number|Signal Name |Pin Usage|Pin Name                 |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|IO Register|Signal Integrity|
+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|P1        |            |         |PROG_B                   |         |           |              |          |         |           |         |       |          |           |                |
|P2        |            |DIFFM    |IO_L01P_3                |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P3        |BUS_D0      |IOB      |IO_L01N_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P4        |BUS_A0      |IOB      |IO_L02P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P5        |BUS_D1      |IOB      |IO_L02N_3/VREF_3         |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P6        |            |IBUF     |IP                       |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P7        |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P8        |BUS_A1      |IOB      |IO_L03P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P9        |BUS_A3      |IOB      |IO_L03N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P10       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P11       |BUS_A2      |IOB      |IO_L04P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P12       |BUS_A4      |IOB      |IO_L04N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P13       |            |         |VCCINT                   |         |           |              |          |         |           |         |1.2    |          |           |                |
|P14       |            |IBUF     |IP                       |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P15       |            |DIFFM    |IO_L05P_3                |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P16       |BUS_D2      |IOB      |IO_L05N_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P17       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P18       |BUS_D4      |IOB      |IO_L06P_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P19       |BUS_D3      |IOB      |IO_L06N_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P20       |BUS_PHASE0  |IBUF     |IP/VREF_3                |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P21       |            |         |VCCO_3                   |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P22       |BUS_A9      |IOB      |IO_L07P_3/LHCLK0         |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P23       |BUS_A8      |IOB      |IO_L07N_3/LHCLK1         |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P24       |BUS_D6      |IOB      |IO_L08P_3/LHCLK2         |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P25       |            |DIFFS    |IO_L08N_3/LHCLK3/IRDY2   |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P26       |BUS_PHASE1  |IBUF     |IP                       |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P27       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P28       |            |DIFFM    |IO_L09P_3/LHCLK4/TRDY2   |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P29       |BUS_D5      |IOB      |IO_L09N_3/LHCLK5         |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P30       |BUS_A7      |IOB      |IO_L10P_3/LHCLK6         |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P31       |BUS_A5      |IOB      |IO_L10N_3/LHCLK7         |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P32       |            |IBUF     |IP                       |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P33       |BUS_A6      |IOB      |IO_L11P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P34       |            |DIFFS    |IO_L11N_3                |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P35       |BUS_D7      |IOB      |IO_L12P_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P36       |BUS_A10     |IOB      |IO_L12N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P37       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P38       |            |         |VCCO_3                   |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P39       |BUS_A11     |IOB      |IO_L13P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P40       |BUS_A12     |IOB      |IO_L13N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P41       |BUS_DMA     |IOB      |IO_L14P_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P42       |BUS_RDY     |IOB      |IO_L14N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |         |       |LOCATED   |NO         |NONE            |
|P43       |            |IBUF     |IP                       |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P44       |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P45       |            |IOB      |IO/VREF_3                |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P46       |            |         |VCCO_3                   |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P47       |BUS_A13     |IOB      |IO_L15P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P48       |BUS_A14     |IOB      |IO_L15N_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P49       |BUS_A15     |IOB      |IO_L16P_3                |TRISTATE |LVCMOS25*  |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P50       |BUS_R_W     |IOB      |IO_L16N_3                |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |IFD      |       |LOCATED   |YES        |NONE            |
|P51       |            |IBUF     |IP                       |UNUSED   |           |3             |          |         |           |         |       |          |           |                |
|P52       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P53       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P54       |            |IBUF     |IP                       |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P55       |PROM_CS     |IOB      |IO_L01P_2/CSO_B          |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P56       |            |DIFFS    |IO_L01N_2/INIT_B         |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P57       |            |DIFFMI   |IP_L02P_2                |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P58       |SDIO_DETECT |IBUF     |IP_L02N_2                |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P59       |            |         |VCCO_2                   |         |           |2             |          |         |           |         |2.50   |          |           |                |
|P60       |BUS_RESET   |IBUF     |IO_L03P_2/DOUT/BUSY      |INPUT    |LVCMOS25*  |2             |          |         |           |IFD      |       |LOCATED   |YES        |NONE            |
|P61       |EXTSPI_DIN  |IOB      |IO_L03N_2/MOSI/CSI_B     |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P62       |PBIO49      |IOB      |IO_L04P_2                |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P63       |BUS_IRQ     |IBUF     |IO_L04N_2                |INPUT    |LVCMOS25*  |2             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P64       |            |DIFFM    |IO_L05P_2                |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P65       |BUS_NMI     |IBUF     |IO_L05N_2                |INPUT    |LVCMOS25*  |2             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P66       |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P67       |            |         |VCCINT                   |         |           |              |          |         |           |         |1.2    |          |           |                |
|P68       |BUS_INTOUT  |IOB      |IO_L06P_2                |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P69       |BUS_DMAOUT  |IOB      |IO_L06N_2                |BIDIR    |LVCMOS25*  |2             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P70       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P71       |BUS_INTIN   |IBUF     |IP_L07P_2                |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P72       |BUS_DMAIN   |IBUF     |IP_L07N_2/VREF_2         |INPUT    |LVCMOS25*  |2             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P73       |            |         |VCCO_2                   |         |           |2             |          |         |           |         |2.50   |          |           |                |
|P74       |EXTSPI_CS_N0|IOB      |IO_L08P_2/D7/GCLK12      |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P75       |EXTSPI_CS_N1|IOB      |IO_L08N_2/D6/GCLK13      |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P76       |SRAM_D<4>   |IBUF     |IO/D5                    |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P77       |PBIO46      |IOB      |IO_L09P_2/D4/GCLK14      |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P78       |            |DIFFS    |IO_L09N_2/D3/GCLK15      |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P79       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P80       |BUS_7M      |IBUF     |IP_L10P_2/RDWR_B/GCLK0   |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P81       |            |DIFFSI   |IP_L10N_2/M2/GCLK1       |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P82       |            |DIFFM    |IO_L11P_2/D2/GCLK2       |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P83       |            |DIFFS    |IO_L11N_2/D1/GCLK3       |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P84       |SRAM_A<5>   |IOB      |IO/M1                    |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P85       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P86       |SRAM_A<6>   |IOB      |IO_L12P_2/M0             |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P87       |EXTSPI_DOUT |IBUF     |IO_L12N_2/DIN/D0         |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P88       |            |         |VCCO_2                   |         |           |2             |          |         |           |         |2.50   |          |           |                |
|P89       |PBIO45      |IOB      |IO_L13P_2                |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P90       |SRAM_D<3>   |IBUF     |IO_L13N_2                |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P91       |SDIO_PROTECT|IBUF     |IP                       |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P92       |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P93       |            |DIFFM    |IO_L14P_2/A23            |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P94       |SRAM_NWE    |IOB      |IO_L14N_2/A22            |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P95       |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P96       |            |DIFFM    |IO_L15P_2/A21            |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P97       |SRAM_D<6>   |IBUF     |IO_L15N_2/A20            |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P98       |            |IOB      |IO/VREF_2                |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P99       |SRAM_A<12>  |IOB      |IO_L16P_2/VS2/A19        |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P100      |SRAM_A<10>  |IOB      |IO_L16N_2/VS1/A18        |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P101      |            |IBUF     |IP                       |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P102      |SRAM_A<11>  |IOB      |IO_L17P_2/VS0/A17        |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P103      |EXTSPI_SCLK |IOB      |IO_L17N_2/CCLK           |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P104      |            |         |DONE                     |         |           |              |          |         |           |         |       |          |           |                |
|P105      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P106      |            |DIFFM    |IO_L01P_1/A16            |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P107      |SDA         |IBUF     |IO_L01N_1/A15            |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P108      |SCL         |IBUF     |IO_L02P_1/A14            |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P109      |            |DIFFS    |IO_L02N_1/A13            |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P110      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P111      |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P112      |            |DIFFM    |IO_L03P_1                |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P113      |TDO_SOFT    |IOB      |IO_L03N_1/VREF_1         |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P114      |            |         |VCCO_1                   |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P115      |            |DIFFM    |IO_L04P_1                |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P116      |SRAM_D<0>   |IBUF     |IO_L04N_1                |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P117      |            |         |VCCINT                   |         |           |              |          |         |           |         |1.2    |          |           |                |
|P118      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P119      |SRAM_NCS<1> |IOB      |IO_L05P_1/A12            |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P120      |SRAM_D<5>   |IBUF     |IO_L05N_1/A11            |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P121      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P122      |SRAM_A<3>   |IOB      |IO_L06P_1                |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P123      |SRAM_A<2>   |IOB      |IO_L06N_1/VREF_1         |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P124      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P125      |            |         |VCCO_1                   |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P126      |SRAM_A<1>   |IOB      |IO_L07P_1/A10/RHCLK0     |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P127      |SRAM_NOE    |IOB      |IO_L07N_1/A9/RHCLK1      |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P128      |CLK_EN      |IOB      |IO_L08P_1/A8/RHCLK2      |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P129      |SRAM_D<7>   |IBUF     |IO_L08N_1/A7/RHCLK3/TRDY1|INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P130      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P131      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P132      |CLK_EXT1    |IOB      |IO_L09P_1/A6/RHCLK4/IRDY1|OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P133      |            |DIFFS    |IO_L09N_1/A5/RHCLK5      |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P134      |SRAM_A<13>  |IOB      |IO_L10P_1/A4/RHCLK6      |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P135      |SRAM_A<14>  |IOB      |IO_L10N_1/A3/RHCLK7      |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P136      |            |IBUF     |IP/VREF_1                |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P137      |SRAM_A<16>  |IOB      |IO_L11P_1/A2             |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P138      |SRAM_A<15>  |IOB      |IO_L11N_1/A1             |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P139      |            |DIFFM    |IO_L12P_1                |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P140      |PBIO0       |IOB      |IO_L12N_1/A0             |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P141      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P142      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P143      |            |         |VCCO_1                   |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P144      |PBIO1       |IOB      |IO_L13P_1                |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P145      |PBIO2       |IOB      |IO_L13N_1                |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P146      |PBIO3       |IOB      |IO_L14P_1                |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P147      |            |DIFFS    |IO_L14N_1                |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P148      |            |IBUF     |IP                       |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P149      |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P150      |PBIO4       |IOB      |IO_L15P_1/HDC            |OUTPUT   |LVCMOS25*  |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P151      |            |DIFFS    |IO_L15N_1/LDC0           |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P152      |            |DIFFM    |IO_L16P_1/LDC1           |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P153      |            |DIFFS    |IO_L16N_1/LDC2           |UNUSED   |           |1             |          |         |           |         |       |          |           |                |
|P154      |TMS_SOFT    |IBUF     |IP                       |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P155      |            |         |TMS                      |         |           |              |          |         |           |         |       |          |           |                |
|P156      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P157      |            |         |TDO                      |         |           |              |          |         |           |         |       |          |           |                |
|P158      |            |         |TCK                      |         |           |              |          |         |           |         |       |          |           |                |
|P159      |TDI_SOFT    |IBUF     |IP                       |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P160      |            |DIFFM    |IO_L01P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P161      |SRAM_NCS<0> |IOB      |IO_L01N_0                |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P162      |            |DIFFM    |IO_L02P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P163      |SRAM_D<1>   |IBUF     |IO_L02N_0/VREF_0         |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P164      |            |DIFFM    |IO_L03P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P165      |            |DIFFS    |IO_L03N_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P166      |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P167      |            |DIFFM    |IO_L04P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P168      |            |DIFFS    |IO_L04N_0/VREF_0         |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P169      |            |IBUF     |IP                       |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P170      |            |         |VCCINT                   |         |           |              |          |         |           |         |1.2    |          |           |                |
|P171      |SRAM_D<2>   |IBUF     |IO_L05P_0                |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P172      |            |DIFFS    |IO_L05N_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P173      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P174      |            |DIFFMI   |IP_L06P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P175      |            |DIFFSI   |IP_L06N_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P176      |            |         |VCCO_0                   |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P177      |            |DIFFM    |IO_L07P_0/GCLK4          |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P178      |            |DIFFS    |IO_L07N_0/GCLK5          |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P179      |SRAM_A<4>   |IOB      |IO/VREF_0                |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P180      |            |DIFFM    |IO_L08P_0/GCLK6          |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P181      |CLK_EXT0    |IOB      |IO_L08N_0/GCLK7          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P182      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P183      |SYSCLK      |IBUF     |IP_L09P_0/GCLK8          |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P184      |TCK_SOFT    |IBUF     |IP_L09N_0/GCLK9          |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P185      |            |DIFFM    |IO_L10P_0/GCLK10         |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P186      |SRAM_A<9>   |IOB      |IO_L10N_0/GCLK11         |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P187      |            |IOB      |IO                       |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P188      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P189      |            |DIFFM    |IO_L11P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P190      |            |DIFFS    |IO_L11N_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P191      |            |         |VCCO_0                   |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P192      |            |DIFFM    |IO_L12P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P193      |            |DIFFS    |IO_L12N_0/VREF_0         |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P194      |            |IBUF     |IP                       |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P195      |            |         |VCCAUX                   |         |           |              |          |         |           |         |2.5    |          |           |                |
|P196      |SRAM_A<8>   |IOB      |IO_L13P_0                |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P197      |SRAM_A<7>   |IOB      |IO_L13N_0                |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P198      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
|P199      |            |DIFFM    |IO_L14P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P200      |            |DIFFS    |IO_L14N_0/VREF_0         |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P201      |            |         |VCCO_0                   |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P202      |            |DIFFM    |IO_L15P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P203      |ONE_WIRE_ID |IBUF     |IO_L15N_0                |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P204      |N_BUS_IO_SEL|IBUF     |IP                       |INPUT    |LVCMOS25*  |0             |          |         |           |IFD      |       |LOCATED   |YES        |NONE            |
|P205      |            |DIFFM    |IO_L16P_0                |UNUSED   |           |0             |          |         |           |         |       |          |           |                |
|P206      |SRAM_A<0>   |IOB      |IO_L16N_0/HSWAP          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P207      |            |         |TDI                      |         |           |              |          |         |           |         |       |          |           |                |
|P208      |            |         |GND                      |         |           |              |          |         |           |         |       |          |           |                |
+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


