# Flags

Each flag can individually be set or cleared on the Processor Status Register ('P'). Cleared flags will show up with a normal background. Set flags will show with an inverse background.

Notes:

- The legacy commands R? and S?, where? is a flag name (C,Z,I,D,B,R,V,N) has been left in.

Commands to set a flag:

Command | Description
SEC | Set Carry
SEZ | Set Zero
SEI | Set Interrupts Disabled
SED | Set Decimal (BCD) mode
SEB | Set Break
SER | Set Reserved (not used on 6502)
SEV | Set Overflow
SEN | Set Negative

Commands to clear a flag:

Command | Description
CLC | Clear Carry
CLZ | Clear Zero
CLI | Clear Interrupts Disabled
CLD | Clear Decimal (BCD) mode
CLB | Clear Break
CLR | Clear Reserved (not used on 6502)
CLV | Clear Overflow
CLN | Clear Negative