Manx Aztec C 6502 for Apple II ProDOS
Alphabetical (more or less) Utility Commands

Introduction
Assembler, Compiler, Library Utility and Linker
as, asi, as65
cc, cci, c65
lb
ln, ln65
Utilities and Shell Commands
arcv, mkarcv
bye
cat
cd
cmp
cnm
cp
crc
date
debug
df
diff
echo
grep
hd
lock, unlock
ls
mkdir
mv
obd
ord
pr
pwd
rm
set
shift
sqz
tty
ved

Introduction
This is an HTML version of the electronic manual for Manx Aztec C for Apple II ProDOS released as freeware by Phade Software December 1999. The release notes for the electronic manual indicate that the electronic manual contains the same information as the paper manual distributed by Manx Software Systems with the compiler. However, they also indicate that if you are using the AZTEC PLUS release you should use the electronic manual rather than the paper manual supplied by Manx. Welcome to the wonderfully confusing World of Aztec C!
The release notes for the electronic manual also indicate that the following notation in the synopsis part of a manual page only means that the function or utility is available both in UNIX and on the Apple II, but despite that fact, the description for that function or utility may differ between the Apple II and UNIX versions:

            /* Apple // and UNIX function */ or
            /* Apple // and UNIX utility */

The contact information in the release notes for the electronic manual is as follows, but Manx Software Systems have apparently since faded from existence:
Manx Software Systems
P.O. Box 55
Shrewsbury, N.J 07701
Phade Software
Inh. Frank Gadegast
Schierker Strasse 39
1000 Berlin 44 - Germany
The HTML version (this document and others) was produced by Canadian Software Developer Bill Buckels by reformatting the Phade Software UNIX style man pages from the elctronic manual into consolidated HTML documents after converting these from Apple II text to IBM text. The original format has been preserved as much as practically possible, and the content of the Phade Software electronic manual remains apparently intact and unaltered in its transition to HTML.
The main benefits of the HTML version are that you can view the information in the man pages on a single HTML document using a web browser in the relative comfort of a modern user interface and can use your web browsers "Find on this Page" feature to search through the content to easily locate information using your own search criteria. This is much easier than using the unix style man utility which can only search on key topics and will only display a single topic at a time.
Licence and Disclaimer
This is a derivative work and as such the licencing by the original authors applies. Bill Buckels makes no claims of ownership whatsoever for the content of this document, and further assumes no liability for the results its use.
You may use the information in this document in any way you find useful (subject to the original authors restrictions and apparently there aren't any), provided that you agree that Bill Buckels has no warranty obligations or liability resulting from said use in any way whatsoever. If you don't agree, don't use this document.
<< Back to Top

NAME arcv, mkarcv
arcv, mkarcv - source dearchiver and archiver
SYNOPSIS

    arcv arcfile                                         /* Apple // Utility */

    mkarcv arcfile

DESCRIPTION

    arcv extracts the source from the archive arcfile, which has been prevously
    created  be mkarcv, placing  the results in seperated  files in the current
    directory.

    mkarcv creates the  archive file  arcfile, placing  it in  the files  whose
    names  it reads from its  standard input. Only on file  name is read from a
    standard input line.

EXAMPLE

    For example, the  file header.arc contains  the source for  all the  header
    files. To create these header files, enter:

             arcv header.arc

    The files will be created in the current directory.

    The  following command  creates the  archive myarc.arc  containing the file
    in.c, out.c, and hello.c:

            mkarcv myarc < myarc.bld

    The names of the three files are contained in the file myarc.bld:

            in.c
            out.c
            hello.c

BUGS

    It's not possible to archive whole subdirectories and arcv can't find files
    with the complete pathname (that means the files for the archive have to be
    in the current directory).

<< Back to Top

NAME as, asi, as65
as, asi, as65 - Aztec C assemblers
SYNOPSIS

    as [-options] prog.asm                        /* Apple // ProDOS utility */

    asi [-options] prog.asm

    The 6502 assembler is named as on native versions of Aztec C65 and as65 on
    cross development versions.

    Relocatable object files are named .r on the MS-DOS cross development version
    of Aztec C65.

DESCRIPTION

    as and asi are  relocating assemblers that  translate an assembly  language
    source  program into  relocatable object  code. The  two assemblers support
    different machines: as accepts assembly language  for a 6502 or 65C02;  asi
    accepts assembly language for a "pseudo machine".

    In  an executable program, an asi-assembled module must be interpreted by a
    routine that is in the Aztec libraries.

    An executable program  can contain  both modules that  have been  assembled
    with as and modules that have been assembled with asi.

    This description has three sections: the first describes how to operate the
    assembler; the  second describes  the assembler's  options; and  the  third
    presents  information  of  interest  to  those  writing  assembly  language
    programs.

     1. OPERATING INSTRUCTIONS

    Operationally, the  two  assemblers  are very  similar.  In  the  following
    paragraphs,  we will use  the name as  when referring to  features that are
    common to both assemblers. When the two assemblers differ, we will say so.

    as is started with a command line of the form

        as [-options] prog.asm

    where [-options] are optionally parameters and prog.asm is the name of  the
    file  to be assembled.  as reads the  source code from  the specified file,
    translates it into object code, and writes the object code to another file.

    1.1 The Source File

    The extension on the source file  name is optional. If not specified,  it's
    assumed to be .asm . For example, with the following command, the assembler
    will assume that the file is test.asm:

        as test

    as will append  .asm to  the source  file name only  if it  doesn't find  a
    period  in the file name. So if the  name of the source file really doesn't
    have an extension, you must assemble it like this:

        as filename.

    The period tells the assembler not to append .asm to the name.

    1.2 The Object File

    By default, the name of the file to which as writes object code is  derived
    from  the name of the source code file, by changing its extension to .o (or
    to  .i, if asi is used). Also by default, the object code file is placed in
    the directory that contains the source code file. For example, the command

        as test.asm

    writes object code  to the  file test.o  (or to  test.i, if  asi is  used),
    placing this file in the current directory.

    You  can explicitly specify the name of  the object code file, using the -O
    option. The  name of  the object  code  file follows  the -O,  with  spaces
    between  the  -O and  the  file name.  For  example, the  following command
    assembles test.asm, writing the object code to the file prog.out:

        as -o prog.out test.asm

    1.3 The Listing File

    The -L option causes the assembler to create a file containing a listing of
    the  program beeing  assembled. The  file is  placed in  the directory that
    contains the  object file;  its derived  from that  of the  object file  by
    changing the extension to .lst .

    1.4 Searching for instxt files

    The  instxt directive tells as to suspend assembly of one file and assemble
    another; when assembly  of the second  file is completed,  assembly of  the
    first continues.

    You  can  make  the assembler  search  for  instxt file  in  a  sequence of
    directories, thus allowing source files and instxt files to be in different
    directories.

    Directories  that are to be searched are defined just as for the compilers;
    that  is,  using  the  -I  assembler  option  or  the  INCLUDE  environment
    variable. Optionally, the compiler can also serach the current directory.

    Directory  search  for a  particular instxt  directive  can be  disabled by
    specifying a  directory name  in  the directive.  In  this case,  just  the
    specified directory is searched.

    1.4.1 The -I option

    A  -I option defines a single directory  to be searched. The directory name
    follows the -I, with no intervening  blanks. For example, the following  -I
    option  tells  the assembler  to search  the include  directory on  the ram
    volume:

        -I/ram/include

    1.4.2 The INCLUDE environment variable

    The INCLUDE environment  variable defines  a directory to  be searched  for
    instxt  files. The example  sets INCLUDE so that  the assembler will search
    for instxt files in the directory /ram/include :

        set INCLUDE=/ram/include

    1.4.3 The search order

    Directories are searched in the following order:

        1.  If the  instxt directive  delimited the  file name  with the double
            quote character, ", the current  directory on the default drive  is
            searched.  If delimited by angle brackets,  < and >, this directory
            isn't automatically searched.

        2.  The directories  defined in -I option  are searched,  in the  order
            listed on the command line.

        3.  The  directory  defined  in  the  INCLUDE  environment  varibale is
            searched.

     2. ASSEMBLER OPTIONS

    The assembler supports the following options:

        Option        Meaning

        -O objname    Send object code to objname.
        -L            Generate listing.
        -C            Disable assembly of 65C02 instructions.  Not supported by
                      asi.
        -ZAP          Delete the source file after assembling it.

     3. PROGRAMMING INFORMATION

    This section discusses  the assembly language  that is supported  by as.  A
    description of the assembly language supported by asi is not available.

    as  supports  the  standard MOS  Technology  syntax: a  program  consist of
    sequence of statements, each of which is in the standard MOS Tech form; and
    the   assembler  supports   the  MOS   Tech  mnemonics   for  the  standard
    instructions. as  supports  some  of  the MOS  Tech  directives  and  their
    mnemonics; it also supports others, as defined below.

    The  following paragraphs define  in more detail  the language supported by
    as.

    3.1 Statement Syntax

        [label] [opcode] [arguments] [[;]comment]

    where the brackets "[...]" indicate an optional element.

    3.2 Labels

    A  statement's label field defines a symbol to the assembler and assigns it
    a value. If present, the symbol name  begins in column one. If a  statement
    is  not  labeled, then  column  one must  be  blank, tab,  or  asterisk. An
    asterisk denotes a comment line.

    Normally, the symbol in a label field is assigned as its value the  address
    at  which the statement's  code will be placed.  However, the equ directive
    can be used to create  a symbol and assign it  some other value, such as  a
    constant.

    A  label can contain  up to 32  characters. Its first  character must be an
    alphabetic character or  one of  the special characters  '_' or  '.' .  Its
    other  characters can  be alphabetic  characters, digits,  '_', or  '.' . A
    label followed by '#' is declared external.

    The cc compiler places  a '_' character  at the end of  all labels that  it
    generates.

    3.3 Opcodes

    The assembler supports the standard MOS Tech instruction mnemonics for both
    the 6502  and 65C02  processors.  The directives  it supports  are  defined
    below.

    3.4 Arguments

    A  statement's argument  can specify  a register,  a memory  location, or a
    constant.

    A memory location can be referenced using any of the standard 6502 or 65C02
    addressing modes, and using the standard MOS Tech syntax.

    A  memory location reference or a  constant can be an expression containing
    any of the following operators:

        *   multiply
        /   divide
        +   add
        -   substract
        #   constant
        =   constant
        <   low byte of expression
        >   high byte of expression

    Expression  are  evaluated from  left  to right  with  no precedence  as to
    oprator or parantheses.

    3.5 Constants

    The  default  base  for  numeric  constants  is  decimal.  Other  bases are
    specified by the following prefixes or suffixes:

        Base    Prefix    Suffix

        2       %         b,B
        8       @         o,O,q,Q
        10      null,&    null
        16      $         h,H

    A  character constant consist of the character, preceded by a single quote.
    For example: 'A .

    3.6 Directives

    The following paragraphs describe the directives that are supported by  the
    assembler.

    END              end

        The end directive defines the end of the source statements.

    CSEG                       cseg

        The  cseg  directive  selects  a  module's  code  segment:  information
        generated  by statements that follow a  cseg directive is placed in the
        module's code  segment, until  another segment-selection  directive  is
        encountered.

    DSEG                       dseg

        The  dseg  directive  selects  a  module's  data  segment:  information
        generated  by statements that follow a  dseg directive is placed in the
        module's data  segment, until  another segment-selection  directive  is
        encountered.

    EQU              symbol    equ

        The equ directive creates a symbol named symbol (if it doesn't  already
        exist), and assigns it the value of the expression expr.

    PUBLIC                     public   [,...]

        The  public  directive  identifies  the  specified  symbols  as  having
        external  scope. If  a specified symbol  was created  within the module
        that's being assembled (by being defined in a statement's label field),
        this  directive allows it to be accessed  by other modules. If a symbol
        was  not  created  within  the  module  that's  being  assembled,  this
        directive  tells the  assembler that  the symbol  was created  and made
        public in another module.

    BSS                        bss      ,

        The bss  directive creates  a symbol  named symname  and reserves  size
        bytes  of space  for it in  the uninitialized data  segment. The symbol
        cannot be accessed by other modules.

    GLOBAL                     global   ,

        The  global directive creates a symbol named symname that other modules
        can access using the global and public directives.

        If other modules create symnam  using just the global directives,  then
        symnam  will be located in a program's uninitialized data area. In this
        case, the amount of space reserved  in this area for symnam will  equal
        the largest value specified by the size fields in the global statements
        that define symnam.

        If other modules define in a public statement, but none of them  create
        symnam  (by specifying it in a label  field), then symnam will still be
        located in the uninitialized  data segment and  space will be  reserved
        for it as defined above.

        If  one of the modules both define  symnam using a public statement and
        creates the symbol by specifying it in a label field, then symnam  will
        be  located in the program's code or  data segment and no space will be
        reserved for it in the uninitialized data segment.

    ENTRY                      entry

        The  entry directive  defines the  symbol symnam  as being  a program's
        entry point.

        When a program is linked, the linker normally places a jump instruction
        at  the  program's data  base  address. If  the  linker found  a module
        containing an entry directive,  it sets the target  of the jump to  the
        location  that was specified in the last entry directive that it found;
        otherwise, it sets the  target to the beginning  of the program's  code
        segment.

    FCB              [label]   fcb      <value>[,<value>...]

        Each value in an fcb directive causes one or more bytes of memory to be
        allocated  and then initialized  to the specified  value. The memory is
        allocated in the currently active segment (code, or data, as defined by
        the last segement-selection directive).

    FCC              [label]   fcc      "string"

        The fcc  directive  allocates a  filed  that  has the  same  number  of
        characters  as are  in string,  and places string  in it.  The field is
        placed in the currently-active segment.

    RMB              [label]   rmb       <expr>

        The rmb  directive  reserves  a  lield containing  expr  bytes  in  the
        currently-active segment. The contents of the field is not defined.

    INSTXT                     instxt    <file>
                               instxt    "file"
                               instxt    /file/

        The instxt directive causes  the assembler to  suspend assembly of  the
        current  source file  and to assemble  the source that's  in file. When
        done, the assembler will continue assembling the original file.

        The assembler can serach for a file in several directories. If file  is
        surrounded by quotes or by slashes, the assembler will begin the search
        at the current directory; it  will search the directories specified  in
        the  -I  option  and  the  INCLUDE  environment  variable.  If  file is
        surrounded by <>,  the assembler will  search just the  -I and  INCLUDE
        directories.

DIAGNOSTICS

    If the  assembler fails  they return -1 as  there value that,  for example,
    tells shell-scripts to stop immediatly.

SEE ALSO
cc, ln, set
<< Back to Top

NAME bye
bye - exit to monitor
SYNOPSIS

    bye                                                  /* Apple // utility */

DESCRIPTION

    bye tranfers control of the processor  to the Apple monitor program  that's
    in  ROM, by  jumping to  location $FF65.  To return  to the  SHELL from the
    monitor, enter the command

            3D0G

    On machines having  the autostart ROM,  you can also  reenter the SHELL  by
    hitting the reset key.

<< Back to Top

NAME cat
cat - catenate and print
SYNOPSIS

    cat [file] [file] ...                       /* Apple // and UNIX utility */

DESCRIPTION

    cat reads  each file  in sequence  and  writes it  to its  standard  output
    device.  If  no files  are  specified, cat  reads  from its  standard input
    device.

    Each argument can specify  a complete or partial  file name, in the  normal
    manner.

    By  default, cat's  standard input and  output devices are  assigned to the
    console. Either or both can also  be redirected to another device or  file,
    if desired, in the normal fashion.

    cat is a built-in SHELL command.

EXAMPLE

    cat hello.c
        Writes hello.c to the screen.

    cat hello.c input.c > cat.out
        Writes hello.c and input.c to cat.out.

    cat
        Copies typed characters to the screen.

    cat > ../newfile
        Copies typed characters to ../newfile.

    cat < /stdio/printf.c > tmp.c
        Equivalent to cat /stdio/printf.c > tmp.c

SEE ALSO
cp
<< Back to Top

NAME cc, cci, c65
cc, cci, c65 - Aztec C compilers
SYNOPSIS

    cc [-options] filename.c                      /* Apple // ProDOS utility */

    cci [-options] filename.c

    The 6502 compiler is named cc on native versions of Aztec C65 and c65 on
    cross development versions.

    Relocatable object files are named .r on the MS-DOS cross development version
    of Aztec C65.

DESCRIPTION

    cc translates C source code into native 6502 assembly language source code.
    cci  translates C source  code into assembly language  source for a "pseudo
    machine"; in an executable program,  cci-compiled code must be  interpreted
    by a special Aztec C routine.

    The compilers were implemented according to the language description in the
    Kernighan and Ritchie book "The C Programming Language".

    This description of the compilers is divided into three subsections:  which
    describe how to use the compilers, compiler options and error processing.

    To  the operator and programmer, the two compilers are very similar. In the
    discussion that follows, we will use  the name cc when describing  features
    that are common to both compilers. Where differences exist, we will say so.

     1. COMPILER OPERATING INSTRUCTIONS

    cc is invoked by a command of the form:

        cc [-options] filename.c

    where [-options] specify optional parameters, and filename.c is the name of
    the file containing  the C  source program.  Options can  appear either  or
    after the name of the C source file.

    The compiler reads C source statements from the input file, translates them
    to assembly language source, and writes the result to another file.

    When the compiler is done, it by default activates the as assembler (cci by
    defaults  starts the asi assembler). The assemblers translates the assembly
    language source to relocatable  object code, writes  the result to  another
    file,  and deletes the  assembly language source file.  The -A option tells
    the compiler not to start the assembler.

    1.1 The C source file

    The extension on the source file  name is optional. If not specified,  it's
    assumed  to be .c .  For example, with the  following command, the compiler
    will assume the file name is text.c :

        cc text

    The compiler will append .c to the source file name only if it does find  a
    period  in the file name. So if the  name of the source file really doesn't
    have an extension, you must compile it like this:

        cc filename.

    The period in the name prevents the compiler from appending .c to the name.

    1.2 The ouput files

    1.2.1 Creating an object code file

    Normally,  when  you  compile  a  C  program  you  are  interested  in  the
    relocatable object code for the program,  and not in its assembly  language
    source.  Because  of this,  the compiler  by  defaults writes  the assembly
    language  source  for  a  C  program  to  an  intermediate  file  and  then
    automatically  starts  the  assembler. The  assembler  then  translates the
    assembly language source to relocatable object code, writes this code to  a
    file, and erases the intermediate file.

    By default, the object code generated by a cc-started assembly is sent to a
    file whose name is derived from that of the file containing the C source by
    changing  its  extension to  .o (the  default  extension for  a cci-started
    assembly is .i).  This file is  placed in the  directory that contains  the
    source file. For example, if the compiler is started with the command

        cc prog.c

    the file prog.o will be created, containing the relocatable object code for
    the program.

    The  name  of   the  file  containing   the  object  code   created  by   a
    compiler-started  assembler  can  also  be  explicitly  specified  when the
    compiler is  started, using  the  compiler's -O  option. For  example,  the
    command

        cc -O myobj.rel prog.c

    compiles  and assembles the C source that's in the file prog.c, writing the
    object code to the file myobj.rel .

    When the compiler  is going  to automatically  start the  assembler, it  by
    default  writes  the assembly  language source  to  a temporary  file named
    ctmpxxx.xxx, where the x's are  replaced by digits in  such a way that  the
    name  becomes  unique.  This  temporary file  is  placed  in  the directory
    specified by  the environment  variable CCTEMP.  If this  variable  doesn't
    exist, the file is placed in the directory specified by the current default
    prefix.

    When CCTEMP  exist,  the fully-qualified  name  of the  temporary  file  is
    generated  by  simply  prefixing its  value  to the  ctmpxxx.xxx  name. For
    example if CCTEMP has the value

        /RAM/TEMP/

    then the temporary file is placed in the TEMP directory on the RAM volume.

    If you are interested in the  assembly language source, but still want  the
    compiler  to start the assembler, specify the  option -T when you start the
    compiler. This will cause the compiler to send the assembly language source
    to  a file  whose name is  derived from that  of the file  containing the C
    source by changing its extension to .asm . The C source statements will  be
    included  as commanets  in the assembly  language source.  For example, the
    command

        cc -T prog.c

    compiles and assembles prog.c, creating the file prog.asm and prog.o .

    1.2.2 Creating just an assembly language file

    There  are  some  programs  for  which  you  don't  want  the  compiler  to
    automatically start the assembler. For example, you may want to modify  the
    assembly  language generated by  the compiler for  a particular program. In
    such cases, you can  use the compiler's -A  option to prevent the  compiler
    from starting the assembler.

    When  you compile a program using the  -A option, you can tell the compiler
    name and  location  of the  file  to which  it  should write  the  assembly
    language source, using the -O option.

    If  you don't use the  -O option but the -A  option, the compiler will send
    the assembly language source to a file  whose name is derived from that  of
    the C source file changing the extension to .asm and place this file in the
    same directory as the one that contains the C source file. For example, the
    command

        cc -A prog.c

    compiles,  without assembling, the  C source that's  in prog.c, sending the
    assembly language source to prog.asm . As another example, the command

        cc -A -O temp.a65 prog.c

    compiles, without assembling, the  C source that's  in prog.c, sending  the
    assembly language source to the file temp.a65 .

    When  the -A option is  used, the -T option  causes the compiler to include
    the C source statements as comments in the assembly language source.

    1.3 Searching for #include files

    You can  make the  compiler search  for  #include files  in a  sequence  of
    directories,  thus allowing source files and #include files to be contained
    in different directories.

    Directories can be  specified with  the -I  compiler option,  and with  the
    INCLUDE  environment variable. The compiler itself also selects a few areas
    to search. The maximum number of searched areas is eight.

    If the file name in the #include statement specifies a directory, just that
    directory is searched.

    1.3.1 The -I option

    A  -I option defines a single directory to be searched. The area descriptor
    follow the -I, with  no intervening blanks. For  example, the following  -I
    option  tells  the compiler  to  search the  include  directory on  the ram
    volume:

        -I/ram/include

    1.3.2 The INCLUDE environment variable

    The  INCLUDE environment variable  also defines a  directory to be searched
    for #include files. For example, the following command sets INCLUDE so that
    the compiler will search for include files in the directory /ram/include:

        set INCLUDE=/ram/include

    1.3.3 The search order for include files

    Directories are searched in the following order:

        1.  If the #include  statement delimited the file  name with the double
            quota character (") the current  directory on the default drive  is
            searched.  If delimited  by angle  brackets (<  >) this  area isn't
            automatically  searched.

        2.  The directories  defined in -I  options are searched,  in the order
            listed on the command.

        3.  The  directory  defined  in  the  INCLUDE  environment  variable is
            searched.

     2. COMPILER OPTIONS

    There  are two types  of options in Aztec  C compilers: machine independent
    and machine dependent. The machine-independent options are provided on  all
    Aztec C compilers. They are identified by a leading minus sign.

    The  Aztec  C  compiler for  each  target has  its  own, machine-dependent,
    options. Such are identified by a leading plus sign.

    The following  paragraphs first  summarize the  compiler options  and  then
    describe them in detail.

    2.1 Summary of options

     2.1.1 MACHINE-INDEPENDENT OPTIONS

        -A                Don't start the assembler when compilation is done.

        -Dsymbol[=value]  Define a symbol to the preprocessor.

        -I dir            Search a directory named dir for #include files.

        -O file           Send output to file.

        -S                Don't print warning messages.

        -T                Include C source statements  in the assembly language
                          code  output  as  comments.  Each  source   statement
                          appears before the assembly code it generates.

        -B                Don't  pause after  every fifth  error to ask  if the
                          compiler should continue.  See the Errors  subsection
                          for details.

        -Enum             Use an expression table having num entries.

        -Lnum             Use an local table having num entries.

        -Ynum             Use a case table having num entries.

        -Znum             Use a literal table having num bytes.

    2.1.2 Special Options for the ProDOS compilers

        +C                Generate 65C02 code (cc only).

        +B                Don't generate the statement "public .begin".

        +L                Turn automatic variables into statics (cc only).

    2.2 Detailed description of the options

    2.2.1 Machine-independent options

    2.2.1.1 The -D option (Define a macro)

    The  -D  option  defines a  symbol  in  the same  way  as  the preprocessor
    directive, #define. It's usage is as follows:

        cc -Dmacro[=text] prog.c

    For example,

        cc -DMAXLEN=1000 prog.c

    is  equivalent  to inserting  the following  line at  the beginning  of the
    program:

        #define MAXLEN 1000

    Since the -D  option causes a  symbol to be  defined for the  preprocessor,
    this can be used in conjunction with the preprocessor directive, #ifdef, to
    selectively include code in a compilation. A common example is code such as
    following:

        #ifdef DEBUG
            printf ("value: %d\n", i);
        #endif

    This  debugging code would be included  in the compiled source by following
    command:

        cc -DDEBUG prog.c

    When no substitution text is specified,  the symbol is defined to have  the
    numerical value 1.

    2.2.1.2 The -I Option (Include another source file)

    The  -I option causes the  compiler to search in  a specified directory for
    files included in the  source code. The name  of the directory  immediately
    follows  the  -I, with  no intervening  spaces. For  more details,  see the
    Compiler Operating Instructions, above.

    2.2.1.3 The -S Option (Be silent)

    The compiler considers some  errors to be genuine  errors and others to  be
    possible errors. For the first type of error, the compiler always generates
    an error message. For  the second, it generates  a warning message. The  -S
    option causes the compiler to not print warning messages.

    2.2.1.4 The Local Symbol Table and the -L Option

    When  the compiler begins processing a compound statement, such as the body
    function or the body of a for loop, it makes entries about the  statement's
    local  symbols in the local  symbol table, and removes  the entries when it
    finishes processing the  statement. If  the table  overflows, the  compiler
    will display a message and stops.

    Be  default, the local symbol  table contains 40 entries.  Each entry is 26
    bytes long, thus by default the table contains 640 bytes.

    You can explicitly define the number  of entries in the local symbol  table
    using the -L option. The number of entries immediately follows the -L, with
    no  intervening spaces. For  example, the following  compilation will use a
    table of 75 entries, or almost 2000 bytes:

        cc -L75 prog.c

    2.2.1.5 The Expression Table and the -E Option

    The compiler uses the expression table  to process an expression. When  the
    compiler  completes its processing of an  expression, it frees all space in
    this table, thus making  the entire table available  for the processing  of
    the  next expression. If the expression  table overflows, the compiler will
    generate error number 36, "no more expression space", and halt.

    By default, the  expression table  contains 80  entries. Each  entry is  14
    bytes long, thus by default the table contains 1120 bytes.

    You  can explicitly  define the number  of entries in  the expression table
    using the -E option. The number of entries immediately follows the -E, with
    no  intervening spaces. For  example, the following  compilation will use a
    table of 20 entries:

        cc -E20 prog.c

    2.2.1.6 The Case Table and the -Y Option

    The compiler uses  the case  table to  process a  switch statement,  making
    entries  in  the table  for the  statement's cases.  When it  completes its
    processing of a switch statement, it frees up the entries for that  switch.
    If this table overflows, the compiler will display error 76 and halt.

    For  example, the following will use a  maximum of four entries in the case
    table:

        switch (a)
        {
            case 0: a += 1;                      /* one */
                    break;
            case 1: switch (x)                   /* two */
                    {
                        case 'a': func1 (a);     /* three */
                                  break;
                        case 'b': func2 (b);     /* four */
                                  break;
                    }                            /* release the last two */
                    a = 5;
            case 3: func2 (a);                   /* total ends at three */
                    break;
        }                                        /* release all entries */

    By default, the table contains 100 entries. Each entry is four bytes  long,
    thus by default, the table occupies 400 bytes.

    You can explicitly define the number of entries in the case table using the
    compiler's -Y option.  The number  of entries immediately  follows the  -Y,
    with  no intervening spaces. For example,  the following compilation uses a
    case table having 50 entries:

        cc -Y50 file

    2.2.1.7 The String Table and the -Z Option

    When  the compiler encounters a "literal" (that is, a character string), it
    places the  string  in the  literal  table.  If this  table  overflow,  the
    compiler will display error 2, "string space exhausted", and halt.

    By default, the literal table contains 2000 bytes.

    You  can explicitly  define the  number of  bytes in  this table  using the
    compiler's -Z option. The number of bytes immediately follows the -Z,  with
    no intervening spaces. For example, the following command will reserve 3000
    bytes for the string table:

        cc -Z3000 prog.c

    2.2.1.8 The Macro/Global Symbol Table

    The compiler stores information about a program's macro and global  symbols
    in  the Macro/Global  Symbol Table. This  table is located  in memory above
    all the other tables used  by the compiler. Its size  is set after all  the
    other  tables have been set.  and hence can't be set  by you. If this table
    overflows, the compiler will display the message "Out of Memory!" and halt.
    You  must recompile, using smaller sizes for the other tables or split your
    C source code.

     2.2.2 PRODOS OPTIONS

    2.2.2.1 The +C Option (Generate 65C02 code - cc only)

    The  +C option causes cc to generate  source for a 65C02 processor. If this
    option isn't used, cc will generate code for a 6502 processor.

    2.2.2.2 The +B Option (Don't generate reference to .begin)

    Normally when compiling a module, the compilers generate a reference to the
    entry  point named .begin . Then when  the module is linked into a program,
    the reference  causes the  linker to  include in  the program  the  library
    module that contains .begin .

    The +B option prevents the compilers from generating this reference.

    For example, if you want to provide your own entry point for a program, and
    its name isn't begin, you should compile the program's modules with the  +B
    option. If you don't, then the program will be bigger than necessary, since
    it will  contain your  entry  point module  and  the standard  entry  point
    module.  In  addition, the  linker by  default sets  at the  program's base
    adress a jump instruction to the program's entry points in several  module,
    it will set the jump to the last encountered.

    2.2.2.3 The +L Option (Turn Autos into Statics - cc only)

    The  +L option causes the  compiler to change the  class of variables whose
    class is automatic  to static.  This can  cause a  significant increase  in
    execution  speed, since it is faster  to adress static variables, which are
    directly addressable, than automatic variables, which are on the stack  and
    must be indirectly addressed.

    Automatic  variables that are declared using the auto keyword, (for example
    auto int i), aren't affected by the +L option: they will remain automatic.

    Also, if a register is available for an automatic variable that is declared
    using the register keyword (for example, register int i), the variable will
    be placed in a register and will not be turned into a static. If a register
    is  not available, however,  such a variable  will be turned  into a static
    variable.

    Like any other static  data, an auto-turned-static  is initialized to  zero
    before the program begins.

    A  function that recursively calls itself may  not work correcty when it is
    compiled with the +L option. For example, the following program will  print
    1  when compiled without the  +L option, and 100  when compiled with the +L
    option.

        main ()
        {
            printf ("%d", qtest ());
        }

        qtest ()
        {
            int i;

            if (++i < 100) qtest (i);
            return (i);
        }

     3. ERROR CHECKING

    Compiler errors come in two varieties  - fatal and not fatal. Fatal  errors
    cause  the compiler  to make  a final  statement and  stop. Running  out of
    memory and finding  no input are  examples of fatal  errors. The  non-fatal
    sort are introduced below.

    The  compiler will report  any error it  finds in the  source file. It will
    first print out a line of code, followed by a line containing the  up-arrow
    (caret)  character. The up-arrow in this  line indicates where the compiler
    was in the source line when it  detected the error. The compiler will  then
    display a line containing the following:

        *   The name of the source file containing the line;
        *   The number of the line within the file;
        *   An error code;
        *   The symbol with causes the error, when appropriate.

    The compiler  writes error  messages to  its standard  output. Thus,  error
    messages  normally  go to  the  console, but  they  can be  associated with
    another device  or a  file  by redirecting  standard  output in  the  usual
    manner. For example,

        cc prog.c                 errors sent to the console;
        cc prog.c > outerr        errors sent to the file outerr.

    The compiler normally pauses after every  fifth error, and sends a  message
    to  its  standard output  asking you  want to  continue. The  compiler will
    continue only if you enter a line beginning with the character 'y'. If  you
    don't  want the  compiler to  pause in this  manner, (if,  for example, the
    compiler's standard output has  been redirected to a  file) specify the  -B
    option when you start the compiler.

    The  compiler is not always able to give a precise description of an error.
    Usally, it must proceed to the next  item in the file to ascertain that  an
    error  was encountered. Once  an error is  found, it is  not obvious how to
    interpret the subsequent code, since  the compiler cannot second-guess  the
    programmer's intentions. This may cause it to flag perfectly good syntax as
    an error.

    If errors arise at  compile time, it  is a general rule  of thumb that  the
    first error should be corrected first. This may clear up some of the errors
    which follow. If the compiler detects  more error with the same symbol,  it
    maybe is only one error (for example, a variable is not declared).

    The  best way to  attack an error  is first to  look up the  meaning of the
    error code.

DIAGNOSTICS

    If the compilation fails the compilers  return -1 as there value that,  for
    example, tells shell-scripts to stop immediatly.

SEE ALSO
as, err, ln, set
<< Back to Top

NAME cd
cd - change current directory
SYNOPSIS

    cd [directory]                              /* Apple // and UNIX utility */

DESCRIPTION

    cd makes cirectory the current directory. If directory isn't specified, the
    current  directory  is set  to  the directory  that's  defined in  the HOME
    environment variable, if this variable exist.

    If  the  specified  directory  doesn't  exist,  the  current  directory  is
    unchanged.

    The directory argument defines the path of directories which must be passed
    trough to reach the new directory. The path can define a complete path from
    the  root directory or  it can define  a partial path,  which is assumed to
    begin at the current directory.

    cd is a built-in SHELL command.

EXAMPLE

    cd /work/io
        The directory /work/io is made the current directory.

    cd subs/io
        The directory  io,  which is  reached  from the  current  directory  by
        passing through the subdirectory subs of the current directory and then
        into io, is made the current  directory. For example, if /work was  the
        current  directory, then  after this  command /work/subs/io  is the new
        current directory.

    cd ..
        The  current directory is set to  the parent directory of the directory
        which was the current before the issuance of this command.

    cd ../include
        The  current  directory is  set to  the directory  which is  reached by
        passing through the parent directory of the directory which was current
        before the issuance of this command and then its include subdirectory.

    cd ../..
        The current  directory is  set to  the directory  which is  reached  by
        passing through the parent directory of the directory which was current
        before the issuance of this command and then to its parent directory.

<< Back to Top

NAME cmp
cmp - file comparison utility
SYNOPSIS

    cmp [-l] file1 file2                        /* Apple // and UNIX utility */

DESCRIPTION

    cmp compares two files an a  character-by-character basis. When it finds  a
    difference,  it displays a message, giving the offset from the beginning of
    the file.

    If the -l  option isn't specified,  the program will  stop after the  first
    difference, displaying a message in the format:

            Files differ: character 10

    If  the  -l option  is specified,  cmp  will list  all differences,  in the
    format:

            decimal-offset hex-offset file1-value file2-value

EXAMPLE

    cmp otst ntst
        Files differ: character 10

    cmp -l otst ntst
         10 a:  00 45
        100 64: 1A 23

<< Back to Top

NAME cnm
cnm - display object file info
SYNOPSIS

    cnm [-sol] file [file ...]                           /* Apple // utility */

DESCRIPTION

    cnm displays the size and symbols  of its object file arguments. The  files
    can  be object modules  created by the  as or asi  assemblers, libraries of
    object modules created by the lb librarian, and 'rsm' files created by  the
    ln linker during the linking of an overlay root.

    For  example, the  following displays the  size and symbols  for the object
    module sub1.o, the library c.lib, and the 'rsm' file root.rsm:

            cnm sub1.o c.lib root.rsm

    By default, the information is sent to the console. It can be redirected to
    a  file or device  in the normal  way. For example,  the following commands
    send information about sub1.o to the display and to the file dispfile:

            cnm sub1.o
            cnm sub1.o > dispfile

    The first line listed by cnm for an object module has the following format:

            file (module): code:cc  data:dd  udata:uu  total:tt(0xhh)

    where

            * file is the name of the file containing the module.
            * module is the name of the  module; if the module is unamed,  this
              field and its surrounding parentheses aren't printed.
            * cc  is the  number of  bytes  in the  module's code  segment,  in
              decimal.
            * dd  is the  number  of bytes  in  the module's  initialized  data
              segment  in decimal. * uu is the  number of bytes in the module's
              uninitialized data segment, in decimal.
            * tt is the total number of  bytes in the module's three  segments,
              in decimal.
            * hh is the total number of  bytes in the module's three  segments,
              in hexadecimal.

    If cnm displays information  about more than one  module, it displays  four
    totals  just  before it  finishes,  listing the  sum  of the  sizes  of the
    modules' code segments, initialized  data segments, and uninitialized  data
    segments, and the sum of the sizes of all segments of all modules. Each sum
    is in decimal, the total of all segments is also given in hexadecimal.

    The -s option tells cnm to display just the sizes of the object modules. If
    the  option isn't specified, cnm also displays information about each named
    symbol in the object modules.

    When cnm  displays information  about the  module's named  symbols, the  -l
    option  tells cnm to  display each symbol's information  on a seperate line
    and to display all  of the characters  in a symbol's  name. If this  option
    isn't  used, cnm displays  the information about several  symbols on a line
    and only displays the first eight characters of a symbol's name.

    The  -o option tells cnm to prefix each line generated for an object module
    with the name  of the file  containing the  module and the  module name  in
    parentheses  (if the module is named). If this option isn't specified, this
    information is listed just once for each module: prefixed to the first line
    generated for the module.

    The  -o  option is  useful when  using  cnm in  combination with  grep. For
    example, the  following commands  will display  all information  about  the
    module perror in the library c.lib:

            cnm -o c.lib > tmp
            grep perror tmp

    cnm displays information about  an module's named  symbols, that is,  about
    the  symbols that begin with something other than a dollar sign followed by
    a digit. For  example, the symbol  quad is named,  so information about  it
    would  be displayed, the  symbol .0123 is unnamed,  so information about it
    would not be displayed.

    For each named symbol in a module, cnm displays its name, a two-  character
    code  specifying its  type, and  an associated  value. The  value displayed
    depends on the type of the symbol.

    If the first character of  a symbol's type code  is lower case, the  symbol
    can  only be accessed by the module, that  is, it's local to the module. If
    this character is upper  case, the symbol is  global to the module:  either
    the  module has defined the symbol and  is allowing other modules to access
    it ar the module  needs to access  the symbol, which must  be defined as  a
    global or public symbol in another module. The type codes are:

            ab    The  symbol  was   defined   using  the   assembler's  EQUATE
                  directive, The  value  listed is  the  equated value  of  its
                  symbol.

                  The compile doesn't generate symbols of this type.

            pg    The symbol is in the code segment. The value is the offset of
                  the symbol within the code segment.

                  The compiler generates this  type symbol for function  names.
                  Static  functions are local to the function, and so have type
                  pg, all other  functions are global,  that is, callable  from
                  other programs, and hence have type Pg.

            dt    The symbol is in  the initialized  data segment. The value is
                  the offset of the symbol from the start of the data segment.

                  The compiler generates symbols  of this type for  initialized
                  variables  which  are declared  outside any  function. Static
                  variables are local to the program  and so have type dt,  all
                  other  variables are  global, that is,  accessable from other
                  programs, and hence have type Dt.

            ov    When an overlay is being linked and that overlay itself calls
                  another  overlay, this tpe of symbols can appear in the 'rsm'
                  file for the overlay that is being linked. It indicates  that
                  the  symbol is defined  in the program that  is going to call
                  the overlay that is being linked.

                  The  value is the offset of  the symbol from the beginning of
                  the physical segment that contains it.

            un    The symbol is used but  not defined  within the  program. The
                  value has no meaning.

                  In   assembly  language  terms,  a  type  of  Un  (the  U  is
                  capitalized) indicates that  the symbol is  the operand of  a
                  public  directive and  that it  is perhaps  referenced in the
                  operand field of some statements, but that the program didn't
                  create the symbol in a statement's label field.

                  The  compiler  generates Un  symbols  for functions  that are
                  called but not defined within the program, for variables that
                  are  declared to be extern and  that are actually used within
                  the program,  and  for  uninitialized,  global  dimensionless
                  arrays.  Variables which are declared  to be extern but which
                  are not  used  within the  program  aren't mentioned  in  the
                  assembly  language source file generated  by the compiler and
                  hence don't appear in the object file.

            bs    The symbol is in the uninitialized data segment. The value is
                  the space reserved for the symbol.

                  The  compiler generates bs  symbols for static, uninitialized
                  variables which are declared outside all functions and  which
                  aren't dimensionless arrays.

                  The  assembler generates bs symbols for symbols defined using
                  the bss assembler directive.

            Gl    The symbol is in the uninitialized data segment. The value is
                  the space reserved for the symbol.

                  The   compiler   generates   Gl   symbols   for   non-static,
                  uninitialized  variables  which  are  declared  outside   all
                  functions and which aren't dimensionless arrays.

                  The  assembler  generates Gl  symbols for  variables declared
                  using the global directive which have a non- zero size.

<< Back to Top

NAME cp
cp - copy files
SYNOPSIS

    cp [-f] infile outfile                      /* Apple // and UNIX utility */

    cp [-f] file1 [file2 ...] dir

DESCRIPTION

    cp copies files, and  their attributes. The first  form of the command,  as
    shown  above, copies infile to outfile. The second copies file1, file2, ...
    into the directory named dir.

    The -f option causes cp to  automatically overwrite any existing files.  If
    this  option isn't specified and if a file to be created already exists, cp
    will ask if you want it overwritten.

    On an Apple // cp is a built-in SHELL command.

EXAMPLE

    The following  command copies  the  file hello.c  that  is in  the  current
    directory to the file newfile.c in the /source directory:

            cp hello.c /source/newfile.c

    The next command copies all ".c" files in the /arc directory to the current
    (ie, the ".") directory:

            cp /arc/*.c .

SEE ALSO
chmod, lock, unlock
BUGS

    cp doesn't copy read-protected files. It only creates them.

<< Back to Top

NAME crc
crc - Utility for generating the CRC for files
SYNOPSIS

    crc file1 file2 ...                         /* Apple // and UNIX utility */

DESCRIPTION

    crc computes a number, called the CRC, for the specified files.

    The CRC for a file is entirely dependent on the file's contents, and it  is
    very  unlikely that  two files whose  contents are different  will have the
    same CRCs.  Thus, crc  can be  used to  determine whether  a file  has  the
    expected contents.

EXAMPLE

    As  an example of the usage of  crc, the following command computes the crc
    of all files whose extension is .c:

            crc *.c

<< Back to Top

NAME date
date - display date and time
SYNOPSIS

    date                                                 /* Apple // utility */

DESCRIPTION

    Displays the date and time.

    date is a built-in SHELL command.

<< Back to Top

NAME debug
debug - set debug mode
SYNOPSIS

    debug                                                /* Apple // utility */

DESCRIPTION

    To debug a SHELL-activated program using the monitor program That's in ROM,
    first  enter the  debug command,  and then enter  the command  to start the
    program. The SHELL will load the program, perform i/o redirection and  pass
    arguments to it if necessary, then, when it sees that the debug command was
    entered, it will jump to the monitor.

    When you're done debugging return to the SHELL by entering the command:

            3D0G

    The debug command affects only the next program that the SHELL starts. That
    is, for each program that you want to debug, you must first enter the debug
    command and then enter the command to start the program.

    debug is a built-in SHELL command.

<< Back to Top

NAME df
df - display volume info
SYNOPSIS

    df [/vol]                                            /* Apple // utility */

DESCRIPTION

    Displays information about disk space utilization.

    The optional parameter  /vol defines the  disk of interest.  It can be  the
    name  of a file or directory. In  this case, information is displayed about
    the disk that contains the specified file or directory.

    /vol can  also  be  the  single character  '/'  (ie,  specify  the  SHELL's
    simulated  root  directory  of  the  entire  file  system).  In  this case,
    information is displayed about all on-line disks.

    If /vol isn't specified, and if  the current directory isn't the  simulated
    root  directory of the file system, information is displayed about the disk
    that contains the current directory.

    If /vol isn't specified, and if the current directory is the simulated root
    directory  of the file  system, information is  displayed about all on-line
    disks.

EXAMPLE

    The following command displays information about the disk that contains the
    current directory:

            df

    The next command displays information about the /ram disk:

            df /ram

    The next command displays information about all on-line disks:

            df /

<< Back to Top

NAME diff
diff - source file comparison utility
SYNOPSIS

    diff [-b] file1 file2                       /* Apple // and UNIX utility */

DESCRIPTION

    diff is  a program,  similar to  the UNIX  program of  the same  name,  hat
    determines  the  difference between  two files  containing text.  file1 and
    file2 are the names of the files to be compared.

     1. THE -B OPTION

        The  -b option causes diff to  ignore trailing blanks (spaces and tabs)
        and to consider strings of blanks to be identical. If this option isn't
        specified,  diff considers two lines to be  the same only if they match
        exactly.

        diff will never consider blanks to match a null string, regardless of
        whether -b was used or not.

     2. THE CONVERSION LIST

        diff writes, to its standard output, a "conversion list" that describes
        the changes that need to be made to file1 to convert it into file2. The
        list is organized into a sequence of items, each of which describes one
        operation that must be performed on file1.

    2.1 Conversion Items

        There are three types of operations that can be specified in a
        conversion list item:

            *    adding lines to file1 from file2;
            *    deleting lines from file1;
            *    replacing (changing) file1 lines with file2 lines.

        A conversion list item consists a letter describing the operation to be
        performed:  'a' for  adding lines, 'd'  for deleting line,  and 'c' for
        changing lines.

        Preceding and following  the letter  are the  numbers of  the lines  in
        file1  and file2, respectively, that are  affected by the command. If a
        range of lines in  a file are affected,  just the beginning and  ending
        line numbers are listed, seperated by a comma.

        So one line of the output of diff will look like

            file1line [,file1to] [letter] file2line [,file2to]
            [><] diffline

    2.1.2 The affected lines

        As mentioned above, the lines affected by a conversion item's operation
        are listed after the item's command line. The affected lines from file1
        are listed first, flagged with a  preceding '<'. The come the  affected
        lines  from file2,  flagged with a  preceding '>'. The  file1 and file2
        lines are seperated by the line ---.

        Since no lines  from file1 are  affected by an  'add' conversion  item,
        only  the file2 lines that  will be added to  file1 are listed, and the
        seperator line '---' is omitted.

     3. DIFFERENCES BETWEEN THE UNIX AND MANX VERSION OF DIFF

        The Manx und UNIX versions of  diff are actually most similar when  the
        latter  program is invoked  with the -h  option. As with  the UNIX diff
        when used with  the -h option,  the Manx diff  works best when  changed
        stretches  are  short  and  well  sperated,  and  works  with  files of
        unlimited length.

        Unlike the UNIX diff, the Manx  diff doesn't support the options e,  f,
        or  h and requires that both operands  to diff be actual files. Because
        of this, the Manx version of  diff doesn't support the features of  the
        UNIX  version  which allows  one operand  to be  a directory  name, (to
        specify a file  in that  directory having the  same name  as the  other
        operand),  and which  allows one operand  to be '-'  (to specify diff's
        standard input instead of a file).

<< Back to Top

NAME echo
echo - echo arguments
SYNOPSIS

    echo [arg1] [arg2] ...                               /* Apple // utility */

DESCRIPTION

    echo writes its arguments, seperated by blanks and terminated by a newline,
    to its standard output device.

    The  ouput thus goes, by default, to  the screen. It can also be redirected
    to another device or file in the normal manner.

    echo is a built-in SHELL command.

<< Back to Top

NAME grep
grep - pattern-matching program
SYNOPSIS

    grep [-cflnv] pattern [files]               /* Apple // and UNIX utility */

DESCRIPTION

    grep is a  program, similar  to the  UNIX program  of the  same name,  that
    searches  files for lines containing a  pattern. By default, such lines are
    written to grep's standard output.

     1. INPUT FILES

        The files parameter is a list of files to be searched. If no files  are
        specified, grep searches its standard input. Each file name can specify
        a single file to be searched.

     2. OPTIONS

        The following options are supported:

            v    print all lines that don't match the pattern

            c    print just the  name of  each file  and the number of matching
                 lines that it contained

            l    print the names of just the files that contain matching lines

            n    precede each matching line that's printed by its relative line
                 number within the file that contains it

            f    a character in the pattern will match both its upper and lower
                 case equivalent

     3. PATTERNS

        A  pattern  consists  of  a  limited  form  of  regular  expression. It
        describes a set of character strings, any of whose members are said  to
        be matched by the regular expression.

        Some  patterns  match  just  a single  character,  others,  which match
        strings, can be constructed from those that match single characters. In
        the  following paragraphs, we'll first describe the patterns that match
        a single character, and  then describe patterns  that match strings  of
        characters.

    3.1 Matching single characters

        The patterns that match a single character are these:

            *    an ordinary  character (that  is,  one other  than the special
                 characters described below) matches itself

            *    a period (.)  is a  pattern that matches any  character except
                 newline.

            *    a non-empty string of  characters enclosed in square brackets,
                 [], matches aby one character in that string

                 If the string begins with the caret character,(^), the regular
                 expression matches  any character  except the  other  enclosed
                 characters  and newline. The '^' has this special meaning only
                 if its the first character of the string.

                 The minus character, (-), can be  used to indicate a range  of
                 consecutive   ASCII  characters  (   [0-9]  is  equivalent  to
                 [0123456789] ).

            *    A backslash, (\), followed  by a special character matches the
                 special character itself. The special characters are:

                    .,  *, [, and \, which are always special, except when they
                    appear in square backets, ([]).

                    caret, (^), which is special when it is at the beginning of
                    an entire regular expression (as discussed in 3.4) and when
                    it immediately  follows  the  left  of  a  pair  of  square
                    brackets.

                    $,  which  is  special  at the  end  of  an  entire regular
                    expression (discussed in 3.4).

    3.2 Matching character string

        Patterns can  be  concatenated. In  this  case, the  resulting  pattern
        matches  strings  whose  substrings  match  each  of  the  concatenated
        patterns.

    3.3 Matching repeating characters

        A pattern can be built by appending an asterick, (*), to a pattern that
        match  a single character.  The resulting pattern  matches zero or more
        occurences of the single-character pattern.

    3.4 Matching strings that begin or end lines

        An entire pattern may  be constrained to  match only character  strings
        that  occur at  the beginning  or the  end of  a line,  by beginning or
        ending the pattern with the character '^' or '$', respectively.

EXAMPLE

    4.1 Simple string matching

        The following command will search the files file1.txt and file2.txt and
        print the lines containing the word heretofore:

            grep heretofore file1.txt file2.txt

        If you aren't interested in the specific lines of these files, but just
        want to know the names of the file containing the word heretofore,  you
        could enter

            grep -l heretofore file1.txt file2.txt

        The  above  two  examples  ignore lines  in  which  heretofore contains
        capital letters,  such as  when  it begins  a sentence.  The  following
        command will cover this situation:

            grep -lf heretofore file1.txt file2.txt

        grep processes  all  option  at  once,  so  multiple  options  must  be
        specified in one dash parameter. For example, the command

            grep -l -f heretofore file1.txt file2.txt

        won't work.

    4.2 The special character '.'

        Suppose  you want to find  all lines in the  file prog.c that contain a
        four-character string whose first and last characters are 'm' and  'n',
        respectively,  and  whose other  characters you  don't care  about. The
        command

           grep m..n prog.c

        will do the trick, since the  special character '.' matches any  single
        character.

    4.3 The backslash character

        There  are occasions when you want to find the character '.' in a file,
        and don't want grep to consider it to be special. In this case, you can
        use  the backslash character,  (\), to turn off  the special meaning of
        the next character.

        For example,  suppose  you  want  to find  all  lines  containing  .PP.
        Entering

            grep .PP prog.doc

        isn't  adequate, because it will find  lines such as THE APPLICATION OF
        since the '.' matches the letter 'A'. But if you enter

            grep /.PP prog.doc

        grep will print just what you want.

        The backslash character can be used to turn off the special meaning of
        any special character. For example,

            grep \\n prog.c

        finds all lines in prog.c containing the string '\n'.

    4.4 The dollar sign and caret ($ and ^)

        Suppose you want to find the number of the line on which the definition
        of the function add occure in the file arith.c. Entering

            grep -n add arith.c

        isn't good,  because it  will print  lines in  which add  is called  in
        addition  to the line you're interested in. Assuming that you begin all
        function definitions at the beginning of a line, you could enter

            grep ^add arith.c

        to accomplish purpose.

        The character '$' is a companion to '^', and stands for 'the end of the
        line'. So if you  want to file  all lines in file.doc  that end in  the
        string time, you could enter

            grep time$ file.doc

        And the following will finds all lines that contain just .PP:

            grep ^\.PP$

    4.5 Using brackets

        Suppose  that you  want to  find all  lines in  the file  file.doc that
        begins with a digit. The command

            grep ^[0123456789] file.doc

        will do just that. This command can be abbreviated as

            grep ^[0-9] file.doc

        And if you wanted to print all lines that don't begin with a digit, you
        could enter

            grep ^[^0-9] file.doc    or
            grep -v ^[0-9] file.doc

    4.6 Repeated characters

        Suppose you want  to find  all lines in  the file  prog.c that  contain
        strings  whose first character is 'e'  and whose last character is 'z'.
        The command

            grep e.*z prog.c

        will do that. The  'e' matches an  'e', the '.*'  matches zero or  more
        arbitrary characters, and the 'z' matches a 'z'.

     5. DIFFERENCES BETWEEN THE MANX AND UNIX VERSION OF GREP

        The Manx and UNIX version of grep differ in the options they accept and
        the patterns they match.

    5.1 Option differences

        The option -f is supported only by the Manx grep.
        The option -b and -s are supported only by the UNIX grep.

    5.2 Pattern differences

        Basically, the patterns accepted by the Manx grep are a subset of those
        accepted by the UNIX grep.

        The Manx grep doesn't allow a regular expression to be surrounded by
        '\(' and '\)'.

        The Manx grep doesn't accept the construct '\{m\}'.

        The Manx  grep doesn't  allow a  right bracket,  ']', to  be  specified
        within brackets.

        Quoted strings can't be passed to the Manx grep. For example, the Manx
        grep won't accept

            grep 'this is a fine kettle of dish' file.doc

<< Back to Top

NAME hd
hd - hex dump utility
SYNOPSIS

    hd [-r] [+n[.]] file1 ...                            /* Apple // utility */

DESCRIPTION

    hd displays the  contents of  one or  more files in  hex and  ascii to  its
    standard output.

    file1, file2, ... are the names of the files to be displayed.

    +n  specifies the offset into  the file where the  display is to start, and
    defaults to the beginning of the file.

    if +n  is followed  by a  period,  n is  assumed to  be a  decimal  number,
    otherwise,  it's  assumed to  be hexdecimal.  Each  file will  be displayed
    beginning at the last specified offset.

EXAMPLE

    hd +16b oldtest newtest +0 junk

        Displays  the data forks of the files oldtest and newtest, beginning at
        offset 0x16b, and of the file names junk beginning at its first byte.

    hd -r +1000. tstfil

        Displays the contents of the resource fork of tstfil, beginning at byte
        1000.

<< Back to Top

NAME lb
lb - object file librarian
SYNOPSIS

    lb library [options] [mod1 mod2 ...]                 /* Apple // utility */

    Relocatable object files are named .r on the MS-DOS cross development version
    of Aztec C65.

DESCRIPTION

    lb is a program that creates  and manipulates libraries of object  modules.
    The modules must have been created by the Manx assembler.

     1 THE ARGUMENTS TO LB

    1.1 The library arguments

        When started, lb acts upon a single library file. The first argument to
        lb (library, in the  synopsis) is the name  of this file. The  filename
        extension for library is optional, if not specified, it's assumed to be
        .lib.

    1.2 The option argument

        There are  two types  of option  argument: function  code options,  and
        qualifier  options. These options  will be summarized  in the following
        paragraphs, and then described in detail below.

    1.2.1 Function code options

        When lb is started, it performs one function on the specified  library,
        as  defined by the options argument. The functions that lb can perform,
        and their corresponding option code, are:

            Function                         Code

            create a library                 (no code)
            add modules to a library         -a, -i, -b
            list library modules             -t
            move library within a library    -m
            replace modules                  -r
            delete modules                   -d
            extract modules                  -x
            ensure modules uniqueness        -u
            help                             -h

        In the synopsis, the options argument is surrounded by square brackets.
        This  indicates  that  the  argument  is  optional,  if  a  code  isn't
        specified, lb assumed that a library is to be created.

    1.2.2 Qualifier options

        In addition to a  functions code, the  options argument can  optionally
        specify  a qualifier, that  modifies lb's behavior  as it is performing
        the requested function. The qualifiers and their codes are:

            verbose                          -v
            silent                           -s

        The  qualifier can  be included  in the  same argument  as the function
        code, or as a seperate argument.

    1.3 The mode arguments

        The  arguments mod1, mod2, etc are the  names of the object modules, or
        the files  contianing  these modules,  that  lb  is to  use.  For  some
        functions,  lb  requires  an  object module  name,  and  for  others it
        requires the name of a file containing and object module. In the latter
        case,  the file's extension  is optional, if  not specified, lb assumes
        that it's .o.

    1.4 Reading arguments from another file

        lb has a special argument, -f filename, that causes it to read  command
        line arguments from the specified file. When done, it continues reading
        arguments from the command line. Arguments  can be read from more  than
        one file, but the file specified in a -f filename argument can't itself
        contain a -f filename argument.

     2. BASIC FEATURES OF LB

        In this section we want to describe tha basic features of lb. With this
        knowledge in hand, you can start using lb, and then read about the rest
        of the features of lb at your leisure.

        The basic  things  you  need to  know  about  lb, and  which  thus  are
        described in this section, are:

            *    How to create a library
            *    How to list the name of modules in a library
            *    How modules get their names
            *    Order of modules in a library
            *    Getting lb arguments from a file

    2.1 Creating a library

        A  library is created by starting lb with a command line that specifies
        the name of the library file to  be created and the names of the  files
        whose  object modules  are to  be copied  into the  library. It doesn't
        contain a function code, and it's this absence of a function code  that
        tells lb that it is to create a library.

        An  object module file from  which modules are read  into a new library
        can itself be a library created by lb. In this case, all the modules in
        the library are copied into the new library.

    2.1.1 The temporary library

        When  lb creates  a library or  modifies an existing  library, it first
        creates a  new library  with  a temporary  name.  If the  function  was
        successful  performed, lb erases  the file having the  same name as the
        specified library, and then renames the new library, giving it the name
        of  the specified library. Thus, lb makes  sure it can create a library
        before erasing an existing one.

        Note that there must be room on  the disk for both the old library  and
        the new.

    2.2 Getting the table of contents for a library

        To list the names of the modules in a library, use lb's -t option.  The
        list  will include some  **DIR** entries. These  identify blocks within
        the library tthat  contain control  information. They  are created  and
        deleted automatically as needed, and cannot be changed by you.

    2.3 How modules get their names

        When  a module is copied into a library from a file containing a single
        object module  (that  is, from  object  module generated  by  the  Manx
        assembler),  the name of the module  within the library is derived from
        the name of the  input file by deleting  the input file's volume,  path
        and  extension components.  An input file  can itself be  a library. In
        this case, a module's name in the  new library is the same as its  name
        in the input library.

    2.4 Order in a library

        The  order of modules in a library is important, since the linker makes
        only a single pass through a library when it is searching for  modules.
        When  lb creates  a library,  it places modules  in the  library in the
        order in which it reads them.

        The ord utility program can be  used to create a library whose  modules
        are optionally sorted.

    2.5 Getting lb arguments from a file

        For libraries containing many  modules, it is frequently  inconvenient,
        if not impossible, to enter all the arguments to lb on a single command
        line. In this case,  lb's -f filename  feature can be  of use: when  lb
        finds  this  option, it  opens the  specified  file and  starts reading
        command arguments from  it. After  finshing the file,  it continues  to
        scan the command line.

        Arguments  in a -f file can be  seperated by any sequence of whitespace
        characters ('whitespace'  being  blanks,  tabs,  and  newlines).  Thus,
        arguments in a -f file can be on seperate lines, if desired.

        The  lb command  line can  contain multiple  -f arguments,  allowing lb
        arguments to be  read from  several files. A  -f file  can contain  any
        valid  lb  argument, except  another  -f. That  is,  -f files  can't be
        nested.

     3. ADVANCED LB FEATURES

    3.1 Adding modules to a library

        lb allows you to add modules to an existing library. The modules can be
        added before or after a specified module in the library or can be added
        to the beginning or end of the library.

        The options that select lb's add function are:

            Option       Function

            -b target    add modules before the module target
            -i target    same as -b target
            -a target    add modules after the module target
            -b+          add modules to the beginning of the library
            -i           +same as -b+
            -a           +add modules to the end of the library

        In any lb command that selects the add function, the name of the  files
        containing  modules to  be added follows  the add option  code (and the
        target module  name, when  appropriate). A  file can  contain a  single
        module or a library of modules.

        Modules are addes in the order that they are specified. If a library is
        to be added, its modules are added in the order they occur in the input
        library.

    3.2 Moving modules within a library

        Modules  which already  exist in a  library can be  easily moved about,
        using the move option, -m.

        As with the option for adding modules to an existing library, there are
        several forms of move functions:

            Option       Meaning

           -mb target    move modules before the module target
           -ma target    move modules after the module target
           -mb+          move modules to the beginning of the library
           -ma+          move modules to the end of the library

        In the lb command,  the names of  the modules to  be moved follows  the
        'move' option code.

        The  modules are  moved in  the order  in which  they are  found in the
        original library, not in the order in  which they are listed in the  lb
        command.

    3.3 Deleting modules

        Modules can be deleted from a library using lb's -d option. The command
        for deletion has the form

            lb libname -d mod1 mod2 ...

        where mod1, mod2, ... are names of the modules to be deleted.

    3.4 Replacing modules

        The lb option 'replace' is used to replace one module in a library with
        one or more other modules.

        The 'replace' option has the form

            lb libname -r target

        where  target is the  name of the  module being replaced.  In a command
        that  uses the 'replace'  option, the names of  the files whose modules
        are to replace the  target module follow the  'replace' option and  its
        associated  target module. Thus, an lb  command to replace a module has
        the form:

            lb library -r target mod1 mod2 ...

    3.5 Uniqueness

        lb allows libraries to be  created containing duplicate modules,  where
        one module is a duplicate of another if it has the same name.

        The  option  -u causes  lb to  delete duplicate  modules in  a library,
        resulting in  a  library  in  which each  module  name  is  unique.  In
        particular,  the -u option causes lb to scan through a library, looking
        at module  names. Any  modules found  that are  duplicates of  previous
        modules are deleted.

    3.6 Extracting modules from a library

        The  lb option  -x extracts  modules from  a library  and puts  them in
        sperated files, without modifying the library.

        The names of the modules to be  extracted follows the -x option. If  no
        modules are specified, all modules in the library are extracted.

        When  a module is extracted,  it's wriiten to a  new file, the file has
        the same name as the module and extension .o.

    3.7 The 'verbose' option

        The 'verbose' option, -v, causes lb to be verbose, that is, to tell you
        what  it's  doing. This  option  can be  specified  as part  of another
        option, or all by itself.

    3.8 The 'silence' option

        The 'silence' option, -s, causes lb to not display its signon  message.
        This  option is especially useful when redirecting the output of a list
        command to a disk file, as described below.

    3.9 Rebuilding a library

        The following commands provide a convenient way to rebuild a library:

            lb exmpl -st > tfil
            lb exmpl -f tfil

        The  first command writes the names of  the modules in exmpl.lib to the
        file tfil.  The second  command  then rebuilds  the library,  using  as
        arguments the listing generated by the first command.

        The -s option to the first command prevents lb from sending information
        to tfil that would foul up the  second command. The names send to  tfil
        entries for the directory blocks, **DIR**, but these are ignored by lb.

    3.10 Help

        The -h option is provided for brief lapses of memory, and will generate
        a  summary of lb functions and options  (same as calling lb without any
        argument). It is producing an output like:

            append/insert:          -[+/-] target
            move module:            -m[+/-] target
            replace module:         -r target
            delete module:          -d target
            uniqueness:             -u
            extract module:         -x [target]
            table listing:          -t
            specify obj extension:  -e

            usage: lb libraryname -[key][position] [posname] [modules] ...

<< Back to Top

NAME ln, ln65
ln, ln65 - Aztec C Linker /* Apple // ProDOS utility */
SYNOPSIS

    ln [-options] file.o [file.o ...] [lib.lib ...]

    The 6502 linker is named ln on native versions of Aztec C65 and ln65 on
    cross development versions.

    Relocatable object files are named .r on the MS-DOS cross development version
    of Aztec C65.

DESCRIPTION

    The ln linker has two functions:

        *   It ties  together the pieces of a program which have been  compiled
            and assembled separately;

        *   It converts the  linked pieces to a format which  can be loaded and
            executed.

    The pieces must have been created by the Manx assembler.

    The first section of this chapter presents a brief introduction to  linking
    and  what the  linker does.  If you  have previous  experience with linkage
    editors, you may wish to continue reading with the second section, entitled
    "Using  the  Linker". There  you  will find  a  concise description  of the
    command format for the linker.

     1. INTRODUCTION TO LINKING

    1.1 Relocatable Object Files

    The object code produced by the  assembler is "relocatable" because it  can
    be  loaded anywhere in memory. One task of the linker is to assign specific
    addresses to the  parts of  the program.  This tells  the operating  system
    where to load the program when it is run.

    1.2 Linking hello.o

    It  is very unusual for a C  program to consist of a single, self-contained
    module. Let's consider a simple  program which prints "hello, world"  using
    the function, printf. The terminology here is precise; printf is a function
    and not an intrinsic feature  of the language. It  is a function which  you
    might  have written,  but it  already happens  to be  provided in  the file
    c.lib . This file is a library  of all the standard i.o functions. It  also
    contains  many support routines  which are called in  the code generated by
    the compiler. These  routines aid in  integer arithmetic, operating  system
    support, etc.

    When  the linker sees that a call to printf was made, it pulls the function
    from the library and combines it with the "hello, world" program. The  link
    command would look like this:

        ln hello.o c.lib

    When  hello.c  was  compiled, calls  were  made to  some  invisible support
    functions in  the library.  So linking  without the  standard library  will
    cause some unfamiliar symbols to be undefined.

    All  programs will need  to be linked with  one of the  versions of c.lib .
    Initially, you  can use  c.lib itself.  Later on,  if you  find that  c.lib
    doesn't suit your requirements, you can use one of the other versions.

    1.3 The Linking Process

    Since the  standard  library contains  only  a limited  number  of  general
    purpose  functions, all but  the most trivial programs  are certain to call
    user-defined functions. It is up to  the linker to connect a function  call
    with the definition of the function somewhere in the code.

    In  the example  given below,  the linker will  find two  function calls in
    file 1. The reference to func1  is "resolved" when the definition of  func1
    is found in the same file. The following command

        ln file1.o c.lib

    will  cause  an error  indicating that  func2 is  an undefined  symbol. The
    reason is that the definition of func2 is in another file, namely file2.o .
    The linkage has to include this file in order to be successful:

        ln file1.o file2.o c.lib

        file1                            file2

        func1 ()                         func2 ()
        {                                {
            printf ("hello, ");              printf ("world");
            return;                          return;
        }                                }

        main ()
        {
            func1 ();
            func2 ();
        }

    1.4 Libraries

    A library is  a collection  of object files  put together  by a  librarian.
    Libraries  intended for use with ln must  be built with the Manx librarian,
    lb.

    All the object  files specified  to the linker  will be  "pulled into"  the
    linkage;  they  are automatically  included in  the final  executable file.
    However, when a library is encountered, it is searched. Only those  modules
    in the library which satisfy a previous function call are pulled in.

    1.5 For example

    Consider  the "hello, world" example. Having looked at the module, hello.o,
    the linker has built  a list of undefined  symbols. This list includes  all
    the  global  symbols  that have  been  referenced but  not  defined. Global
    variables and all function names are considered to be global symbols.

    The list of undefined's  for hello.o includes the  symbol printf. When  the
    linker  reaches the standard library, this is one of the symbols it will be
    looking for. It will  discover that printf is  defined in a library  module
    whose  name also happens to be printf. (There is not any necessary relation
    between the name of a library module and the functions defined within it.)

    The  linker pulls in the printf module in order to resolve the reference to
    the printf function.

    Files are examined in the order in which they are specified on the  command
    line. So the following linkages are equivalent:

        ln hello.o

        ln c.lib hello.o

    Since no symbols are undefined when the linker searches c.lib in the second
    line, no modules are pulled in. It is good practice to leave all  libraries
    at the end of the command line, with the standard library last of all.

    1.6 The Order of Library Modules

    For  the  same  reason,  the  order of  the  modules  within  a  library is
    significant. The linker searches a library once, from beginning to end.  If
    a  module  is pulled  in at  any point,  and that  module introduces  a new
    undefined symbol,  then  that  symbol  is added  to  the  running  list  of
    undefined's.  The linker will  not search the library  twice to resolve any
    references which remain unresolved.  A common error  lies in the  following
    situation:

        module of program             references (function calls)

        main.o                        getinput, do_calc
        input.o                       gets
        calc.o                        put_value
        output.o                      printf

    Suppose we build a library to hold the last three modules of this  program.
    Then our link step will look like this:

        ln main.o proglib.lib c.lib

    But  it is important  that proglib.lib is  built in the  right order. Let's
    assume  that  main()  calls  to  functions,  getinput  ()  and   do_calc().
    getinput()  is defined in the module input.o. It in turn calls the standard
    library function  gets(). do_calc()  is in  calc.o and  calls  put_value().
    put_value() is in output.o and calls printf(). What happens at link time if
    proglib.lib is built as follows?

        proglib.lib       input.o
                          output.o
                          calc.o

    After main.o, the  linker has getinput  and do_calc undefined  (as well  as
    some  other  support functions  in  c.lib). Then  it  begins the  search of
    proglib.lib. It  looks at  the  library module,  input, first.  Since  that
    module  defines getinput, that symbol is taken off the list of undefined's.
    But gets is added to it.

    The symbols do_calc  and gets are  undefined when the  linker examines  the
    module,  output. Since  neither of  these symbols  are defined  there, that
    module is ignored. In  the next module, calc,  the reference to do_calc  is
    resolved but put_value is a new undefined symbol.

    The linker still  has gets  and put_value undefined.  It then  moves on  to
    c.lib,  where  gets  is  resolved.  But  the  call  to  put_value  is never
    satisfied. The error from the linker will look like this:

        Undefined symbol: put_value_

    This means  that the  module defining  put_value was  not pulled  into  the
    linkage.  The reason, as  we saw, was  that put_value was  not an undefined
    symbol when the output module was passed over. This problem would not occur
    with the library built this way:

        proglib.lib       input.o
                          calc.o
                          output.o

    The  standard libraries were put together with  much care so that this kind
    of problem would not arise.

    Occasionally it becomes difficult or impossible to build a library so  that
    all  references are resolved.  In the example, the  problem could be solved
    with the following command:

        ln main.o proglib.lib proglib.lib c.lib

    The second time  through proglib.lib, the  linker will pull  in the  module
    output.  The reason this is not the  most satisfactory solution is that the
    linker has to search the library twice; this will lengthen the time  needed
    to link.

     2. USING THE LINKER

    The general form of a linkage is as follows:

        ln [-options] file.o [file.o ...] [lib.lib ...]

    The linker can create programs having the following types:

        *   PRG programs, which can only be executed in the SHELL environment;

        *   BIN programs, which  can be executed in either in  the SHELL or the
            Basic Interpreter environments;

        *   SYS programs, which are ProDOS system programs.

    By default, the linker creates a PRG program. The +B option makes it create
    a  BIN  program, and  the  +S option  make it  create  a SYS  program. When
    creating a BIN or SYS  program, you will also  have to include the  startup
    routine samain.o in the program.

    2.1 The executable file

    The  name of the executable output file can be selected using the -O linker
    option. If this option isn't used, the  linker will derive the name of  the
    output  file from that of the first object file listed on the command line,
    by deleting its extension. In the default case, the executable file will be
    located  in the directory  in which the  first object file  is located. For
    example,

        ln prog.o c.lib

    will produce the file  prog. The standard library,  c.lib, will have to  be
    included in most linkages.

    A  different output  file can be  specified with  the -O option,  as in the
    following command:

        ln -O program mod1.o mod2.o c.lib

    This command  also  shows how  several  individual modules  can  be  linked
    together. A "module", in this sense, is a section of a program containing a
    limited number of functions, usally related. These modules are compiled and
    assembled separately and linked together to produce an executable file.

    2.2 Libraries

    Several  libraries of object  modules are provided with  the Aztec C65. The
    most freqently-used of these are c.lib, which contains 6502 versions of the
    non-floating  point functions, and  m.lib, which contains  6502 versions of
    the floating  point  functions.  Other libraries  are  provided  with  some
    versions of Aztec C65.

    All  programs must be linked with one of the versions of c.lib. In addition
    to containing  6502 versions  of all  the non-floating  point functions  it
    contains  internal functions  which are called  by compiler-generated code,
    such as functions to perform long arithmetic.

    Programs  that perform floating point operations must be linked with one of
    the version of m.lib, in addition to a version of c.lib. The floating point
    library must be specified on the linker command line before c.lib .

    Libraries  of user modules  can also be  searched by the  linker. These are
    created with the Manx lb program, and must be listed on the linker  command
    line before the Manx libraries.

    For  example,  the  following  links the  module  program.o,  searching the
    libraries mylib.lib, new.lib, m.lib and c.lib for needed modules:

        ln program.o mylib.lib new.lib m.lib c.lib

    Each of the  libraries will be  searched once  in the order  in which  they
    appear on the command line.

    Libraries  can be conveniently specified using  the -L option. For example,
    the following command is equivalent to the one above:

        ln -O program.o -lmylib -lnew -lm -lc

    For more information, see the description of the -L option below.

     3. LINKER OPTIONS

    3.1 Summary of options

    3.1.1 General Purpose Options

        -O file    Write executable code to the file named file.

        -Lname     Search the library name.lib for needed modules.

        -F file    Read common arguments from file.

        -T         Generate a symbol table file.

        -M         Don't issue warning messages.

        -N         Don't abort if there are undefined symbols.

        -V         Be verbose.

    3.1.2 Options for Segment Address Specification

        -B addr    Set the program's base address to the hex value addr.

        -C addr    Set the  starting address of the  program's code  segment to
                   the hex value addr.

        -D addr    Set the  starting address of the  program's data segment  to
                   the hex value addr.

        -U addr    Set the starting offset of the  program's uninitialized data
                   segment to the hex value addr.

    3.1.3 Option for Overlay Usage

        -R         Create a symbol table to be used when linking overlays.

        +C size    Reserve size bytes at end of the program's code segment (the
                   overlay's code segment is loaded here). size is a hex value.

        +D size    Reserve  size  bytes  at  end  of  the  program's  code  and
                   uninitialized data segements (the  overlay's data is  loaded
                   here). size is a hex value.

    3.1.4 Special Options for ProDOS

        +B             Create a BIN program.

        +S             Create a SYS program.

        +H start,end   Define a hole in the program, whose beginning and ending
                       addresses are hex values start and end.

    3.2 Detailed description of the options

    3.2.1 General Purpose Options:

    3.2.1.1 The -O option

    The  -O option can  be used to  specify the name  of the file  to which the
    linker is to write the executable program. The name of this file is in  the
    parameter  that follows the  -O. For example,  the following command writes
    the executable program to the file progout:

        ln -O progout prog.o c.lib

    If this option isn't  used, the linker derives  the name of the  executable
    file from that of the first input file, by deleting its extension.

    3.2.1.2 The -L option

    The  -L option provides  a convenient means  of specifying to  the linker a
    library that is should search, when the extension of the library is .lib.

    The name  of the  library is  derived  by concatenating  the value  of  the
    environment  varibale  CLIB, the  letters  that immediately  follow  the -L
    option, and  the string  .lib. For  example, with  the libraries  subs.lib,
    io.lib,  m.lib and c.lib in a directory specified by CLIB, you can link the
    module prog.o, and have the linker search the libraries for needed  modules
    by entering

        ln prog.o -lsubs -lio -lm -lc

    CLIB  is  set using  the SHELL's  set command.  For example,  the following
    command defines CLIB when the libraries are in the directory /ln/lib:

        set CLIB=/ln/libs/

    Note the terminating slash on the CLIB variable: this is required since the
    linker simply prepends the value of the CLIB variable to the -L string.

    3.2.1.4 The -F option

    -F  file causes the linker to merge the contents of the given file with the
    command line  arguments.  For example,  the  following command  causes  the
    linker  to  create an  executable program  in the  file myprog.  The linker
    includes the  modules  myprog.o, mod1.o  and  mod2.o in  the  program,  and
    searches the libraries mylib.lib and c.lib for needed modules.

        ln myprog.o -F argfile c.lib

    where the file argfile, contains the following:

        mod1.o mod2.o mylib.lib

    The  linker  arguments in  argfile  can be  seperated  by tabs,  spaces, or
    newlines. There are several uses for the -F option. The most obvious is  to
    supply  the names of modules that are frequently linked together. Since all
    the modules named  are automatically  pulled into the  linkage, the  linker
    does  not spend any time  in searching, as with  a library. Furhermore, any
    linker option except -F  can be given in  a -F file. -F  can appear on  the
    command  line more than once, and in any order. The arguments are processed
    in the order in which they are read, as always.

    3.2.1.5 The -T option

    The  -T option creates  a disk file  which contains a  symbol table for the
    linkage. This file  is just  a text  file which  lists each  symbol with  a
    hexadecimal  address. This address is either the entry point for a function
    or the location  in memory  of a  data item. A  perusal of  this file  will
    indicate which functions were actually included in the program.

    The  symbol  table  file  will have  the  same  name as  that  of  the file
    containing the executable program, with extension changed to .sym .

    3.2.1.6 The -M option

    The linker issues  the message "multiply  defined symbol" when  it finds  a
    symbol  that is  defined with  the assembly  language directives  global or
    public in more than one module. The -M option causes the linker to  supress
    this  message  unless  the  symbol  is  defined  in  more  than  one public
    directive.

    To maintain compability with the previous  versions of Aztec C, the  linker
    will  generate  code for  a  variable that  is  defined in  multiple global
    statements and  in  at  most  one public  statement,  and  also  issue  the
    "multiply  defined symbol" message. Thus, if  you use the global and public
    directives in this  way, and don't  want to  get this message,  use the  -M
    option to supress them.

    The  definition of  a symbol  in more that  one public  directives is never
    valid, so the -M option doesn't supress messages in this case.

    3.2.1.7 The -N option

    Normally, the  linker halts  without generating  an executable  program  if
    there  are undefined symbols. The  -N option causes the  linker to go ahead
    and generate an executable program anyway.

    3.2.1.8 The -V option

    The -V option causes the linker to send a progress report of the linkage to
    the screen as each input file is processed. This is useful in tracking down
    undefined symbols and errors which may occur while linking.

    3.2.2 Option for segment address specification

    The linker organizes a program into three segments: code, initialized data,
    and uninitialized data areas. You can define the starting address of  these
    segments  using the -C,  -D, and -U linker  options, respectively. A fourth
    option, -B, will set the "base  address" of the program. These options  are
    followed by the desired offset, in hex.

    By  default, the base address  of a PRG or BIN  program is 0x800, while the
    base address of a SYS program is 0x2000. Also by default, a program's  code
    segment  starts three  bytes after the  base address,  its initialized data
    segment  follows  the  code,  and   its  uninitialized  data  follows   the
    initialized data.

    A  file created by the linker contains  a memory image of the program, from
    its base address through the end  of its code or initialized data  segments
    (whichever  is higher).  This image is  loaded into memory,  with the first
    byte in the file loaded at the program's base address.

    By default, a program is expected  to begin execution at its base  address.
    Most  programs  have  a  startup  routine,  which  performs  initialization
    activities and then calls the program's main function. This entry point  to
    the  startup routine is usually somewhere in  the middle of the program, so
    at the base address the linker will normally set a jump instruction to  the
    entry point.

    You  can explicitly specify that  a label in a module  is an entry point by
    placing the label in  the operand field of  the module's assembly  language
    entry  directive.  For  example,  the crt0  module  in  c.lib  contains the
    function .begin . This label is dclared  in a public directive and also  in
    the  module's entry  directive. When a  C module is  compiled, the compiler
    always generates a reference to .begin;  thus, when the program is  linked,
    ln  will include the crt0() module from c.lib and place a jump to .begin at
    the program's base address.

    If the linker doesn't find  a startup routine when  it links a program,  it
    won't set the jump instruction at the program's base address. In this case,
    if you don't specify a starting  offset for the program's code segment,  it
    will right at the base address.

    For example, the following command sets the base address of prog to 0x4000:

        ln -B 4000 -O prog prog.o -lc

    Because  none  of the  other segment  selection options  were used  in this
    example, the program's code  will begin at offset  0x4003, followed by  its
    initialized data, followed by its uninitialized data.

    In  the next example, the program's base address is set to 0x900 the offset
    of its code, initialized data,  and uninitialized data segments to  0x2000,
    0x2800, and 0x3000, respectively.

        ln -B 900 -C 2000 -D 2800 -U 3000 prog.o -lc

    3.2.3 Options for Overlay Usage

    The  -R option causes the  linker to generate a  file containing the symbol
    table. It's used when linking a program which calls overlays.

    The  name of the symbol  table file is derived  from that of the executable
    file by changing the  extension to .rsm  . The file is  placed in the  same
    directory as the executable file.

    The  linker reserves space in a program between its uninitialized data area
    and its heap, into which the  program's overlay will be loaded. The  amount
    of  space equals the sum of the values  that you define using the +C and +D
    options. For example,

        ln +C 3000 +D 1000 prog.o -lc

    will reserve 0x400 bytes for overlays.

    3.2.4 Special Option for ProDOS

    3.2.4.1 The +B Option

    The +B option  causes the linker  to set the  type of a  file containing  a
    created program to BIN.

    3.2.4.2 The +S Option

    The  +S option  causes the linker  to set the  type of a  file containing a
    created program to SYS and to set the default base address for the  program
    to 0x2000.

    3.2.4.3 The +H option

    The  +H option defines a  "hole", that is an area  of memory into which the
    linker should not place a  program's code or data.  You can create at  most
    four holes in a program using +H options.

    The option has the following form:

        +H start,end

    where  start and end are the addresses,  in hex, of the hole's starting and
    ending addresses.

    For example, suppose  you want  to create a  program, line,  that uses  the
    primary  graphics page (between addresses 0x2000-0x4000) and that begins at
    address 0x800. The following command will link the program:

        ln +H 2000,4000 line.o -lc

    The linker will place as much of the program's code and data as possible in
    the  area between 0x800-0x2000,  and place any additional  code and data in
    the area above 0x4000.

    The linker creates a  program's code segment  by concatenating module  code
    segments,  until and  unless a module's  code overlaps a  reserved area. If
    this occurs, the linker  moves the module's entire  code segment above  the
    reserved  area, in  the first non-reserved  area in which  it will entirely
    fit, and then continues the concatenation of module code segments.

    The  linker creates a program's initialized  data segement in the same way:
    it concatenates  module  initialized data  segments  as much  as  possible,
    without  overlapping  a  reserved  area  and  without  breaking  a module's
    initialized data segment into discontigous pieces.

    Because the linker won't break up a module's code segment or data  segment,
    it's likely that some space below a hole will be left unused by the linker.

DIAGNOSTICS

    If  the linker fails it  return -1  as its value  that, for  example, tells
    shell-scripts to stop immediatly.

SEE ALSO
as, cc, lb, set
<< Back to Top

NAME lock, unlock
lock, unlock - lock and unlock files
SYNOPSIS

    lock file1 file2 ...                                 /* Apple // utility */

    unlock file1 file2 ...

DESCRIPTION

    These commands lock  and unlock the  specified files. When  locked, a  file
    can't be removed, renamed, or written to.

    lock and unlock are built-in SHELL commands.

<< Back to Top

NAME ls
ls - list directory contents
SYNOPSIS

    ls [-option] [name1 name2 ...]              /* Apple // and UNIX utility */

DESCRIPTION

    ls displays information about the  files and directories name1, name2,  ...
    If  no names are specified, ls displays information about all the files and
    directories in the current directory.

    A  name  can  optionally  specify  multiple  files,  using  the   "wildcard
    characters"  * and ?. These  have their standard meaning:  * matches one or
    more characters, and ? matches a single character.

    ls sends the information to its  standard output. This information thus  by
    default  is sent to the  console, but can be redirected  to a file or other
    device in the normal way.

    ls by default displays information in 'short form', listing just the  names
    of  the specified files and directories. You can also specify the -l option
    to cause  ls  to  display  information in  'long  form',  listing  lots  of
    information.

    When  ls sends information in  short form to the  console, the names are in
    columns on the  screen, with  a dash  preceding directory  names. When  the
    information is sent to a file or other device, the names are listed one per
    line, and a directory name isn't by default preceded by a dash.

    ls usally sorts the  list it's going  to display. By  default, the list  is
    sorted  alphabetically, you  can also specify  options to cause  ls to sort
    based on other the list such 'last modified' time and file size, and, for a
    given criteria, to sort in the reverse of the normal order.

    ls supports the following options:

        -l    list in long form.
        -p    When listing  in  short form,  and  redirected, precede directory
              names with a dash.
        -t    sort by 'last-modified' time.
        -s    sort by file size.
        -r    reverse the order of the sort.
        -x    don't sort the file list.

     LONG FORMAT

        The  -l option causes the listing to be made in 'long format', in which
        additional information is displayed  for each file.  In this case,  the
        listing for a file or directory has the following format:

            flags type (aux_type) size date name

        where:

            *    name is the name of the file or directory.
            *    date is the date and time at which it was last modified.
            *    size is the number of bytes that have been written to it.
            *    aux_type is its  aux_type field (for  a  program, this  is its
                 load adress).
            *    type defines the contents of the file or directory.
            *    flags defines other attributes of the file or directory.

     FLAGS FIELD

        The flags field consists  of five characters,  each defines whether  or
        not  the file has a certain attribute. If the file or directory has all
        these attributes,  the falgs  field will  be "debwr".  If the  file  or
        directory   doesn't  have  a   particular  attribute,  the  attribute's
        characters is replaced in the list by a dash, '-'.

        The meanings of the characters are:

            d    deletable.
            e    erasable.
            b    needs to be backed up.
            w    writable.
            r    readable.

     TYPE FIELD

        The type field defines the type of the file. Possible values are:

            PRG    File conatins a  program that  can only  be run in the SHELL
                   environment.
            BIN    File contains a type program that can be run in the SHELL or
                   Basic environment.
            SYS    File contains a ProDOS system file.
            DIR    Directory.
            TXT    This is the  only other  type  of file  created by the Aztec
                   programs.  fopen,  open, and  related functions  also create
                   files or type TXT.

     MOUNTED VOLUMES

        The SHELL pretends that the file system has a root directory, and  that
        all volume directories are subdirectories of this root directory. So to
        diplay the names of all mounted volumes, enter the command

            ls /

        And to display the names of all mounted volumes along with the  numbers
        of the slot and drives that contain them, enter the command

            ls -l /

<< Back to Top

NAME mkdir
mkdir - make directory
SYNOPSIS

    mkdir dirname1 dirname2 ...                 /* Apple // and UNIX utility */

DESCRIPTION

    mkdir creates one or more directories, named dirname1, dirname2, ...

    An empty directory can be  removed with the rm command  on an Apple //  and
    with rmdir command under UNIX.

SEE ALSO
rm
<< Back to Top

NAME mv
mv - move files
SYNOPSIS

    mv [-f] infile outfile                      /* Apple // and UNIX utility */

    mv [-f] file1 [file2 ...] dir

DESCRIPTION

    mv moves files,  and their  attributes. The  original files  then cease  to
    exist.

    The  first form of the  command, as shown above,  copies infile to outfile.
    The second copies file1, file2, ... into the directory named dir.

    The -f option causes mv to  automatically overwrite any existing files.  If
    this  option isn't specified and if a file to be created already exists, mv
    will ask if you want it overwritten.

    In both forms, mv will simply change the name of the original file to  that
    of  the  target  file  if the  two  files  are in  the  same  directory. It
    physically copies  a file  and  then deletes  the  original only  when  the
    directories of the two files differ.

    mv is a built-in SHELL command on an Apple //.

EXAMPLE

    The  following  command  moves the  file  hello.c  that is  in  the current
    directory to the file newfile.c in the /source directory:

        mv hello.c /source/newfile.c

    The next command moves all ".lib" files in the /ln directory to the /pl/lib
    directory:

        mv /ln/*.lib /pl/lib

<< Back to Top

NAME obd
obd - list object code
SYNOPSIS

    obd objfile                                          /* Apple // utility */

DESCRIPTION

    obd lists the loader items  in an object file.  It has a single  parameter,
    which is the name of the object file.

<< Back to Top

NAME ord
ord - sort object module list
SYNOPSIS

    ord [-v] [infile [outfile]]                          /* Apple // utility */

DESCRIPTION

    ord sorts a list of object file names. A library of the object modules that
    is generated from the sorted list by object module librarian, lb, will have
    a minimum number of 'backward references', that is, global symbols that are
    defined in one module and referenced in a later module.

    Since  the specification of a library to the linker causes it to search the
    library just  once,  a  library  having  no  backward  references  need  be
    specified  just once when linking a  program, and a library having backward
    references may need to be specified multiple times.

    infile is the name of  a file containing an  unordered list of file  names.
    These  files contain the object modules that  are to be put into a library.
    If infile isn't specified, this list is read from ord's standard input. The
    file names can be seperated be space, tab, or newline characters.

    outfile  is the name  of the file to  which the sorted  list is written. If
    it's not specified, the list is  written to ord's standard output.  outfile
    can only specified if infile is also specified.

    The  -v option causes ord  to be verbose, sending  messages to its standard
    error device as it proceeds.

SEE ALSO
lb, ln
<< Back to Top

NAME pr
pr - initialize devices
SYNOPSIS

    pr s1 [s2 ...]                                       /* Apple // utility */

DESCRIPTION

    pr initializes the devices that are in  slots s1, s2, ..., by calling  each
    device's ROM.

    pr is a built-in SHELL command.

EXAMPLE

    The  following command  initializes the card  in slot 2  by calling address
    0xC200:

        pr 2

<< Back to Top

NAME pwd
pwd - print working directory
SYNOPSIS

    pwd                                         /* Apple // and UNIX utility */

DESCRIPTION

    pwd prints the name of the current directory.

    The name is  written to pwd's  standard output device.  Hence, the name  is
    printed  on the screen, by default, and can be redirected to another device
    or file, if desired.

    pwd is a built-in SHELL command.

SEE ALSO
cd
<< Back to Top

NAME rm
rm - removes files or directories
SYNOPSIS

    rm file [file ...]                          /* Apple // and UNIX utility */

DESCRIPTION

    rm removes the specified files or directories.

    rm will not remove locked files or non-empty directories.

    Under UNIX rm doesn't remove directories. Locking is handled different.

EXAMPLE

    The following command removes  the files file1.bak  and file2.bak from  the
    current directory:

        rm file1.bak file2.bak

<< Back to Top

NAME set
set - environment variable and exec utility
SYNOPSIS

    set                                                  /* Apple // utility */

    set VAR=string

    set VAR=

    set [-+x] [-+e] [-+n]

DESCRIPTION

    set is used  to examine  and set environment  variables, to  set exec  file
    options, and to enable the trapping of errors by the SHELL.

    set is a built-in SHELL command.

    Displaying and setting of environment variables:

        The  first form listed for set causes set to display the name and value
        of each environment variable.

        The second form assigns string to the environment variable VAR.

        The third form removes the variable VAR from the SHELL environment.

    Setting Exec file options:

        x    Command line logging.  With this  option enabled, before a command
             line  in an exec file  is executed, it's logged  to the screen. By
             default, this option is disabled.

        e    Exit prematurely.  With  this  option  enabled,  a  command  which
             terminates  with a non-zero return code causes the exec file to be
             aborted. By default, this option is enabled.

        n    Non-execution. With  this  option enaabled,  commands  in the exec
             file aren't executed. By default, this option is disabled.

             Preceding  an  option's character  with a  minus sign  enables the
             option, and preceding it with a plus sign disables it.

<< Back to Top

NAME shift
shift - shift exec file variables
SYNOPSIS

    shift [n]                                            /* Apple // utility */

DESCRIPTION

    shift causes the values assigned to an exec file variable to be  reassigned
    to  the next  lower-numbered exec  file variable.  n is  the number  of the
    lowest-numbered variable whose value is  to be reassigned, and defaults  to
    1.

    Thus,  shift causes the exec file variable $1 to be assigned with the value
    of $2, $2 to be assigned with $3, and so on. The original value assigned to
    $1  is lost. When all arguments to the  exec file have been shifted out, $1
    is assigned to the null-string.

    shift is a built-in SHELL command.

EXAMPLE

    The following exec file, del, is  passed a directory as its first  argument
    and the names of files within the directory that are to be removed:

        set j=$1
        shift
        loop i in $*
        rm $j/$i
        eloop

    In  this example, j is an environment variable. The first two statements in
    the exec file save the name of  the directory and then shift the  directory
    name out of the exec file variables.

    The loop then repeatedly calls rm to remove one of the specified files from
    the directory.

    Entering

        del . file1.bak file2.bak

    will remove the files file1.bak and file2.bak from the current directory.

<< Back to Top

NAME sqz
sqz - sqeeze an object library
SYNOPSIS

    sqz file [outfile]                                   /* Apple // utility */

DESCRIPTION

    sqz compresses an object module that was created by the Manx assembler.

    The  first parameter is the  name of the file  containing the module to  be
    compressed.  The second  parameter, which is  optional, is the  name of the
    file to which the compressed module will be written.

    If the  output file  is  specified, the  original  file isn't  modified  or
    erased.

    If  the output file isn't specified, sqz creates the compressed module in a
    file having a  temporary name, erases  the original file,  and renames  the
    output  file to have the  name of the original  file. The temporary name is
    different from the input file name by having the extent .sqz.

    If the output file isn't specified and an error occurs during the  creation
    of the compressed module, the original file isn't erased or modified.

<< Back to Top

NAME tty
tty - terminal emulation program
SYNOPSIS

    tty -sy -bxx                                         /* Apple // utility */

DESCRIPTION

    tty is a terminal emulaion program that allows an Apple // operator to talk
    to  another computer. To the other system, the Apple // will appear to be a
    terminal that supports some of the special features of the ADM-3A terminal.

    tty reads  characters  from  the  keyboard and  writes  them  to  a  serial
    interface.  It  also reads  characters characters  from this  interface and
    writes them to  the console.  This interface  must be  compatible with  the
    Super Serial Card.

    The  -s option defines the number of the slot containing the interface. The
    number immediately  follows the  -s, with  no intervening  spaces. If  this
    option isn't specified, the interface is assumed to be in slot 2.

    The  -b option defines the baud rate of the serial interface. The baud rate
    immediately follows  the -b  option, with  no intervening  spaces. If  this
    option isn't specified, the baud rate is assumed to be 9600.

    To  exit tty, type control-2  (ie, type the '2'  key while holding down the
    control key).

<< Back to Top

NAME ved
ved - vi-like text editor
SYNOPSIS

    ved [-tn] [-gprog] file [+1,c msg]                   /* Apple // utility */

DESCRIPTION

    ved is a screen oriented text editor  that has some of the features of  the
    UNIX vi editor.

    If  ved is  invoked with  a file name,  that file  will be  loaded into the
    memory buffer, otherwise it will be  empty. ved will only edit text  files:
    binary  files cannot be edited.  ved does all its  editing in memory and is
    thus limited in the  size of files  that it will edit.  In ved, the  memory
    buffer is never completely empty. There will always be at least one newline
    in the buffer.

     THE SCREEN

        ved has a  1000 character limit  on the size  of a line.  If a line  is
        longer  than the width of the screen, it will wrap to the next line. If
        a line starts at the bottom of the screen, and its too wide to fit, the
        line  will  not  be  displayed.  Instead,  the  '@'  character  will be
        displayed. Likewise, at the end of  the file, all lines beyond the  end
        will consist only of a single '-' on each line.

        A  number of commands take  a numeric prefix. This  prefix is echoed on
        the status line as it is typed.

     MOVING AROUND IN THE FILE

        The normal mode of ved is command mode. During command mode, there  are
        a  number of ways to  move the cursor around  the screen and around the
        whole file.

            newline      - move to beginning of the next line.
            -            - move to the start of the previous line.
            space        - move to the next character of the line.
            backspace    - move to the previous character.
            0            - move to the first character of this line.
            $            - move to the last character of this line.
            h            - move to the top line of the screen.
            l            - move to the bottom line of the screen.
            b            - move to the first line of the file.
            g            - move to the n'th line of the file.
            /string      - move to hte next occurence of 'string'.

     DELETING TEXT

        When the cursor is in the appropriate spot, there are two commands used
        to delete existing text.

            x     - delete  characters on the  current  line, beginning at  the
                    cursor and continuing up to, but not including the newline.
            dd    - delete lines starting with the current line.

        The  x and dd commands can be prefixed with a number, which defines the
        number of  characters  or  lines  to be  deleted.  If  a  number  isn't
        specified, just one character or line is deleted.

        Note that deleting the last  character of the line (newline  character)
        causes the following line to be appended to the current line.

     INSERTING TEXT

        To  add new text, hitting 'i' key will cause the top line of the screen
        to indicated that you  are now in   mode. To exit insert  mode,
        type  ESCAPE.  To  insert  a control  character  which  means something
        special to ved into a text  file, first type control-v followed be  the
        control  character itself.  Control characters  are displayed  as '^X',
        where X is the appropiate character.

        Typing 'o' will cause a new line to be created below the current  line,
        and  the cursor will be placed on  that line and the editor placed into
         mode.

     MOVING TEXT AROUND

        There are three commands  used for moving  text around. These  commands
        make  use of a 1000 character yank  buffer. The contents of this buffer
        is retained across files.

            yy    - yank lines  starting with the  current  line into  the yank
                    buffer.
            yd    - yank lines starting  with the  current line and then delete
                    them.
            p     - "put" the lines in the yank  buffer after the current line.
                    The yank buffer is not modified.

        A  number can be prefixed to the  yank commands, defining the number of
        lines to  be yanked.  If a  number isn't  specified, just  one line  is
        yanked.

     MISCELLANEOUS COMMANDS

        The  'z' command redraws the screen with the current line in the center
        of the screen.

        The 'r' command repalaces the character under the cursor with the  next
        character typed.

     FILE-RELATED COMMANDS

        When in command mode, if the ':' key is hit, a ':' will be displayed on
        the status  line.  At this  point,  a number  of  special  file-related
        commands may be given.

            :f            - displays info about the current file.
            :w file       - writes the buffer to the specified file name.
            :w            - writes the buffer to the last specfied file.
            :e[!] file    - clears the buffer and prepares file for editing.
            :r file       - reads the named file into the buffer.
            :q[!]         - exits the editor.

        In the above  table, square brackets  surrounding a character  indicate
        that  the  character is  optional. The  exclamation  mark tells  ved to
        execute  the commands in which it's  specified, even if the file that's
        currently being edited has been modified  since it was last written  to
        disk.

     APPLE RELATED INFORMATION

        In  order to use VED on older Apple //'s, which don't have a full ASCII
        keyboard, you  need to  have the  single wire  switch key  modification
        installed.   You  can  then  enter  upper  and  lower  case  alphabetic
        characters using the SHIFT key. You can enter special character used by
        C  programs by typing a control character, that is, by holding down the
        control key  and then  typing another  key. The  following table  lists
        these   control  characters  and  the  characters  to  which  they  are
        translated. In this  table, ^X  is an  abbreviation for  "type X  while
        holding  the  control key  down". The  first column  identifies control
        codes that  you type,  the second  identifies the  characters to  which
        control  codes are translated  when the keyboard is  in lower case mode
        (that is, when the  SHIFT key is off).  The last column identifies  the
        characters  to which control codes are  translated when the keyboard is
        in upper case mode.

            Press:    To get (lower):    To get (upper):

            ^P        `                  @
            ^A        {                  [
            ^E        |                  \
            ^R        }                  ]
            ^N        ~                  ^
            ^C        DEL                _
            ^Q        ESC
            ^U        TAB

        ^U is generated by typing the 'right arrow key'.

        To  exit insert mode, type is ESC key.  In addition to the ESC key, you
        can type control-Q to exit VED's  mode. This is usefull on some
        older  Apple //e's, for which  ESC is intercepted by  the ROM and never
        gets back to VED. Out  of insert mode, the  cursor can be moved  around
        using the space bar to move rigth and the left arrow to move left.

<< Back to Top

© Copyright Phade Software 1999
Released as FreeWare December 1999