one_on_one_gs_patch.dsk
http://204.16.8.40/other/oneonone/one_on_one_gs_patch.dsk

This is a quick patch to EA's One-On-One game to run on a IIgs. Originally, the cracked version quickly crashes after the crack screen.
The reason why is because of an invalid opcode at $8AA. On an 8-bit Apple, it would run this way:

08AA: 54	     ??? (NOP)
08AB: 5C	     ??? (NOP)
08AC:	 A2 00    LDX #$00
08AE: A5 E1    LDA $E1
…

On a 16-bit IIgs, it runs this way:

00/08AA: 54 5C A2       MVN $5C,$A2        
00/08AD: 00 A5          BRK $A5            
00/C074: B8             CLV                
00/C075: 5C 10 00 E1    JMP $E10010        
E1/0010: 5C CC B7 FF    JMP $FFB7CC        
FF/B7CC: 18             CLC                

The 00 aligns to create a BRK instruction, which sends the IIgs into a different bank and it never returns, causing a lock up/loop condition.
The fix is to NOP out the instructions at 08AA and 08AB to cause everything to line back up correctly and run through the routine.

It begs the question as to why it was invalid to begin with… Corrupted original upload? Bug in original cracking job that was never detected?

Edits were done at Track 14 Sector 0C at byte AA:
From: 	54 5C
To:	EA EA

Tested on a ROM1 and ROM3 and seemed to work fine…

datawiz/rich